For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

The GM LAN modules on this vehicle also support DTC Symptom information.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B0012 01 | Driver Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B0012
B0012 02 | Driver Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B0012
B0012 04 | Driver Frontal Deployment Loop Stage 1 Open Circuit | SDM | DTC B0012
B0012 0D | Driver Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B0012
B0012 0E | Driver Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B0012
B0014 01 | LF Side Deployment Loop Short to Battery | SDM | DTC B0014
B0014 02 | LF Side Deployment Loop Short to Ground | SDM | DTC B0014
B0014 04 | LF Side Deployment Loop Open Circuit | SDM | DTC B0014
B0014 0D | LF Side Deployment Loop Resistance Above Threshold | SDM | DTC B0014
B0014 0E | LF Side Deployment Loop Resistance Below Threshold | SDM | DTC B0014
B0015 01 | LF Pretensioner Deployment Loop Short to Battery | SDM | DTC B0015
B0015 02 | LF Pretensioner Deployment Loop Short to Ground | SDM | DTC B0015
B0015 04 | LF Pretensioner Deployment Loop Open Circuit | SDM | DTC B0015
B0015 0D | LF Pretensioner Deployment Loop Resistance Above Threshold | SDM | DTC B0015
B0015 0E | LF Pretensioner Deployment Loop Resistance Below Threshold | SDM | DTC B0015
B0016 01 | Left Roof Rail Initiator 1 Deployment Loop Short to Battery | SDM | DTC B0016
B0016 02 | Left Roof Rail Initiator 1 Deployment Loop Short to Ground | SDM | DTC B0016
B0016 04 | Left Roof Rail Initiator 1 Deployment Loop Open Circuit | SDM | DTC B0016
B0016 0D | Left Roof Rail Initiator 1 Deployment Loop Resistance Above Threshold | SDM | DTC B0016
B0016 0E | Left Roof Rail Initiator 1 Deployment Loop Resistance Below Threshold | SDM | DTC B0016
B0019 01 | Passenger Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B0019
B0019 02 | Passenger Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B0019
B0019 04 | Passenger Frontal Deployment Loop Stage 1 Open Circuit | SDM | DTC B0019
B0019 0D | Passenger Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B0019
B0019 0E | Passenger Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B0019
B001A 01 | Left Front Seat Belt Pretensioner Deployment Loop 2 Short to Battery | SDM | DTC B001A
B001A 02 | Left Front Seat Belt Pretensioner Deployment Loop 2 Short to Ground | SDM | DTC B001A
B001A 04 | Left Front Seat Belt Pretensioner Deployment Loop 2 Open Circuit | SDM | DTC B001A
B001A 0D | Left Front Seat Belt Pretensioner Deployment Loop 2 Resistance Above | SDM | DTC B001A
B001A 0E | Left Front Seat Belt Pretensioner Deployment Loop 2 Resistance Below Threshold | SDM | DTC B001A
B001B 01 | Right Front Seat Belt Pretensioner Deployment Loop 2 Short to Battery | SDM | DTC B001B
B001B 02 | Right Front Seat Belt Pretensioner Deployment Loop 2 Short to Ground | SDM | DTC B001B
B001B 04 | Right Front Seat Belt Pretensioner Deployment Loop 2 Open Circuit | SDM | DTC B001B
B001B 0D | Right Front Seat Belt Pretensioner Deployment Loop 2 Resistance Above | SDM | DTC B001B
B001B 0E | Right Front Seat Belt Pretensioner Deployment Loop 2 Resistance Below Threshold | SDM | DTC B001B
B0021 01 | RF Side Deployment Loop Short to Battery | SDM | DTC B0021
B0021 02 | RF Side Deployment Loop Short to Ground | SDM | DTC B0021
B0021 04 | RF Side Deployment Loop Open Circuit | SDM | DTC B0021
B0021 0D | RF Side Deployment Loop Resistance Above Threshold | SDM | DTC B0021
B0021 0E | RF Side Deployment Loop Resistance Below Threshold | SDM | DTC B0021
B0022 01 | RF Pretensioner Deployment Loop Short to Battery | SDM | DTC B0022
B0022 02 | RF Pretensioner Deployment Loop Short to Ground | SDM | DTC B0022
B0022 04 | RF Pretensioner Deployment Loop Open Circuit | SDM | DTC B0022
B0022 0D | RF Pretensioner Deployment Loop Resistance Above Threshold | SDM | DTC B0022
B0022 0E | RF Pretensioner Deployment Loop Resistance Below Threshold | SDM | DTC B0022
B0023 01 | Right Roof Rail Initiator 1 Deployment Loop Short to Battery | SDM | DTC B0023
B0023 02 | Right Roof Rail Initiator 1 Deployment Loop Short to Ground | SDM | DTC B0023
B0023 04 | Right Roof Rail Initiator 1 Deployment Loop Open Circuit | SDM | DTC B0023
B0023 0D | Right Roof Rail Initiator 1 Deployment Loop Resistance Above Threshold | SDM | DTC B0023
B0023 0E | Right Roof Rail Initiator 1 Deployment Loop Resistance Below Threshold | SDM | DTC B0023
B0052 00 | Deployment Commanded | SDM | DTC B0052
B0053 00 | Deployment Commanded With Loop DTCs Present | SDM | DTC B0053
B0055 00 | Side Air Bag Deployment Commanded | SDM | DTC B0055
B0085 00 | LF Side Impact Sensor | SDM | DTC B0085
B0085 01 | LF Side Impact Sensor Short to Battery | SDM | DTC B0085
B0085 02 | LF Side Impact Sensor Short to Ground | SDM | DTC B0085
B0085 05 | LF Side Impact Sensor Short to Battery or Open | SDM | DTC B0085
B0085 0F | LF Side Impact Sensor Erratic | SDM | DTC B0085
B0085 39 | LF Side Impact Sensor Internal Electronic Failure | SDM | DTC B0085
B0085 3A | LF Side Impact Sensor Incorrect Component Installed | SDM | DTC B0085
B0085 71 | LF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B0085
B0086 00 | RF Side Impact Sensor | SDM | DTC B0086
B0086 01 | RF Side Impact Sensor Short to Battery | SDM | DTC B0086
B0086 02 | RF Side Impact Sensor Short to Ground | SDM | DTC B0086
B0086 05 | RF Side Impact Sensor Short to Battery or Open | SDM | DTC B0086
B0086 0F | RF Side Impact Sensor Erratic | SDM | DTC B0086
B0086 39 | RF Side Impact Sensor Internal Electronic Failure | SDM | DTC B0086
B0086 3A | RF Side Impact Sensor Incorrect Component Installed | SDM | DTC B0086
B0086 71 | RF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B0086
B0158 | Outside Air Temperature Sensor Circuit | BCM | DTC B0158
B0283 | Electric Rear Defrost Circuit | BCM | DTC B0283
B1000 | Electronic Control Unit (ECU) Performance | BCM | DTC B1000
B1000 00 | Electronic Control Unit (ECU) Performance | SDM | DTC B1000
B1001 | Option Configuration Error Variant Not Programmed | BCM | DTC B1001
B1001 01 | Option Configuration Error | SDM | DTC B1001
B1016 | VIN Not Programmed | BCM | DTC B1016
B1015 | VIN Information Error | TDCM | DTC B1015
B1016 | Vehicle Identification Number (VIN) Information Not Programmed | TDCM | DTC B1016
B1019 00 | System Configuration Error | SDM | DTC B1019
B1019 3A | System Configuration Error Incorrect Component Installed | SDM | DTC B1019
B1325 | Device Power Circuit Malfunction | BCM | DTC B1325
B1370 |

• | Device Ignition 1 (ON AND START) Circuit To Battery

• | Device Ignition 1 (ON AND START ) Circuit To Ground Or Open

BCM

DTC B1370

B1370 06 | Device Ignition 1 Circuit Short to Ground | SDM | DTC B1370
B1380 |

• | Device Ignition ACCESSORY Circuit Short To Battery

• | Device Ignition ACCESSORY Circuit Short To Ground Or Open

BCM

DTC B1380

B1395 |

• | Device voltage reference output 1 circuit voltage below threshold

• | Device Voltage Reference Output 1 Circuit Above Threshold

BCM

DTC B1395

B1428 | Ignition Switched Power Relay 1 Circuit | BCM | DTC B1428
B1433 | Ignition Switched Power Relay 2 Circuit | BCM | DTC B1433
B1440 | Power Mode Master Input Circuits Mismatch | BCM | DTC B1440
B1441 |

• | Device Ignition Off, Run, And Crank Circuit Short To Battery

• | Device Ignition Of, Run, And Crank Circuit Short To Ground Or Open

BCM

DTC B1441

B1480 | Battery Rundown Protection Circuit | BCM | --
B1517 |

• | Battery Voltage Below Threshold

• | Battery Voltage Above Threshold

BCM

DTC B1517

B2530 | Front Fog Lamps Control Circuit | BCM | DTC B2530
B2545 | Backup Lamps Circuit | BCM | DTC B2545
B2575 | Headlamp Control Circuit | BCM | DTC B2575
B257A | Headlamp Switch Input Signals Mismatch | BCM | DTC B257A
B2580 | Headlamp High Beam Control Circuit | BCM | DTC B2580
B2585 | Left Park Lamp Control Circuit | BCM | DTC B2585
B2625 | Display Dimming Pulse Width Modulation PWM) Output Circuit | BCM | DTC B2625
B2645 |

• | Ambient Light Sensor Circuit Voltage Below Threshold

• | Ambient Light Sensor Circuit Voltage Above Threshold

BCM

DTC B2645

B2705 | Gearshift Unlock Circuit Short To Ground | BCM | DTC B2705
B2745 | Traction Control System Circuit Short to Ground | EBCM | DTC B2745
B2750 | Horn Relay Coil Circuit | BCM | DTC B2750
B3006 | Hood Ajar Circuit Plausibility Failure | TDCM | DTC B3006
B302A | Telematic Requested Immobilization | TDCM | DTC B302A
B3031 | Security System Controller In Learn Mode | TDCM | DTC B3031
B3055 | No Transponder Modulation or No Transponder | TDCM | DTC B3055
B3060 | Unprogrammed Transponder Identification Code Received | TDCM | DTC B3060
B3130 | All Door Unlock Circuit | BCM | DTC B3130
B3135 | All Door Lock Circuit | BCM | DTC B3135
B3265 | Trunk/Hatch/Lift Glass Release Output Circuit | BCM | DTC B3265
B3445 | Stop Lamp Circuit | BCM | --
B3622 | Steering Wheel Controls Group 1 Signal Circuit Voltage Above Threshold | BCM | DTC B3622
B3715 | Front Wiper Relay Drive Circuit | BCM | DTC B3715
B3794 |

• | Cruise Control Function Request Circuit Signal Invalid

• | Cruise Control Function Request Circuit Actuator Stuck

BCM

DTC B3794

B3873 | Front Washer Relay Circuit | BCM | DTC B3873
B3875 | Wiper High Speed Relay Circuit | BCM | DTC B3875
B3887 | Trailer Left Turn Signal Circuit | BCM | DTC B3887
B3888 | Trailer Right Turn Signal Circuit | BCM | DTC B3888
B3891 | Trailer Fog Lamp Circuit | BCM | DTC B3891
B3922 | Front Wiper Function Select Circuit | BCM | DTC B3922
B3933 |

• | Air Conditioning (A/C) Evaporator Temperature Sensor Circuit Voltage Above Threshold

• | Air Conditioning (A/C) Evaporative Temperature Sensor Circuit Voltage Below Threshold

BCM

DTC B3933

B3935 | Transponder Authentication Error | TDCM | DTC B3935
B3976 | Key Not Programmed | TDCM | DTC B3976
C0035 00 | Left Front Wheel Speed Sensor Circuit Malfunction | EBCM | DTC C0035-C0050
C0035 0F | Left Front Wheel Speed Sensor Circuit Erratic | EBCM | DTC C0035-C0050
C0035 18 | Left Front Wheel Speed Sensor Circuit Signal Amplitude < Minimum | EBCM | DTC C0035-C0050
C0040 00 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0040 0F | Right Front Wheel Speed Sensor Circuit Erratic | EBCM | DTC C0035-C0050
C0040 18 | Right Front Wheel Speed Sensor Circuit Signal Amplitude < Minimum | EBCM | DTC C0035-C0050
C0045 00 | Left Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0045 0F | Left Rear Wheel Speed Sensor Circuit Erratic | EBCM | DTC C0035-C0050
C0045 18 | Left Rear Wheel Speed Sensor Circuit Signal Amplitude < Minimum | EBCM | DTC C0035-C0050
C0050 00 | Right Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0050 0F | Right Rear Wheel Speed Sensor Circuit Erratic | EBCM | DTC C0035-C0050
C0050 18 | Right Rear Wheel Speed Sensor Circuit Signal Amplitude < Minimum | EBCM | DTC C0035-C0050
C0110 04 | Pump Motor Circuit Open Circuit | EBCM | DTC C0110
C0110 61 | Pump Motor Circuit Actuator Stuck | EBCM | DTC C0110
C0131 00 | ABS/TCS System Pressure Circuit Malfunction | EBCM | DTC C0131
C0131 4B | ABS/TCS System Pressure Circuit Malfunction | EBCM | DTC C0131
C0131 5A | ABS/TCS System Pressure Circuit Malfunction | EBCM | DTC C0131
C0161 00 | ABS Brake Switch Circuit | EBCM | DTC C0161
C0186 00 | Lateral Accelerometer Circuit | EBCM | DTC C0186
C0186 1A | Lateral Accelerometer Sensor Offset Error | EBCM | DTC C0186
C0186 3B | Lateral Accelerometer Sensor Self Test Malfunction | EBCM | DTC C0186
C0186 4B | Lateral Accelerometer Circuit Calibration Not Learned | EBCM | DTC C0186
C0186 5A | Lateral Accelerometer Circuit Plausibility Failure | EBCM | DTC C0186
C0196 00 | Yaw Rate Circuit | EBCM | DTC C0196
C0196 1A | Yaw Rate Sensor Offset Error | EBCM | DTC C0196
C0196 3B | Yaw Rate Circuit Internal Self Test Failed | EBCM | DTC C0196
C0196 5A | Yaw Rate Circuit Plausibility Failure | EBCM | DTC C0196
C0252 4A | VSES Sensors Uncorrelated | EBCM | DTC C0252
C0280 00 | Stability System Active Too Long | EBCM | DTC C0280
C0287 00 | Longitudinal Accelerometer Circuit | EBCM | DTC C0287
C0287 11 | Longitudinal Accelerometer Circuit Above Maximum Threshold | EBCM | DTC C0287
C0287 3B | Longitudinal Accelerometer Circuit Internal Self Test Failed | EBCM | DTC C0287
C0292 1A | VSES Combination Sensor Circuits | EBCM | DTC C0292
C0292 39 | VSES Combination Sensor Circuits | EBCM | DTC C0292
C0393 06 | Rear Axle Coupling Solenoid Control Circuit | CCM | DTC C0393
C0393 0B | Rear Axle Coupling Solenoid Control Circuit Current Above Threshold | CCM | DTC C0393
C0394 06 | Rear Axle Coupling Temperature Sensor Circuit | CCM | DTC C0394
C0460 39 | Steering Position Sensor Circuit Malfunction | EBCM | DTC C0460
C0460 42 | Steering Position Sensor Calibration Data Set Not Programmed | EBCM | DTC C0460
C0460 4B | Steering Position Sensor Calibration Not Learned | EBCM | DTC C0460
C0460 5A | Steering Position Sensor | EBCM | DTC C0460
C0460 71 | Steering Position Sensor Data Error | EBCM | DTC C0460
C0460 72 | Steering Position Sensor Circuit Malfunction | EBCM | DTC C0460
C0550 00 | Electronic Control Unit (ECU) Performance | EBCM | DTC C0550
C0550 39 | Electronic Control Unit (ECU) Performance | CCM | DTC C0550
C0551 00 | Option Configuration Error | EBCM | DTC C0551
C0551 41 | Option Configuration Error | EBCM | DTC C0551
C0551 45 | Option Configuration Error Variant Not Programmed | EBCM | DTC C0551
C0551 47 | Option Configuration Error VIN Not Programmed | EBCM | DTC C0551
C0551 4A | Option Configuration Checksum Error | EBCM | DTC C0551
C0551 5A | Option Configuration Error | EBCM | DTC C0551
C0558 4B | Calibration Mismatch | CCM | DTC C0558
C0561 71 | System Disabled Information Stored Invalid Serial Data Received | CCM, EBCM | DTC C0561 or DTC C0561
C0569 00 | System Configuration Error | EBCM | DTC C0569
C0750 | Left Front TPMS Transmitter Battery Voltage Too Low | TPMS | DTC C0750, C0755, C0760, or C0765
C0755 | Right Front TPMS Transmitter Battery Voltage Too Low | TPMS | DTC C0750, C0755, C0760, or C0765
C0760 | Left Rear TPMS Transmitter Battery Voltage Too Low | TPMS | DTC C0750, C0755, C0760, or C0765
C0765 | Right Rear TPMS Transmitter Battery Voltage Too Low | TPMS | DTC C0750, C0755, C0760, or C0765
C0899 00 | Device Power Circuit Low | EBCM | DTC C0899
C0899 03 | Device Voltage Low | CCM | DTC C0899
C0900 00 | Device Power Circuit High | EBCM | DTC C0900
P0008 | Engine Position System Performance Bank 1 | ECM | DTC P0008 or P0009
P0009 | Engine Position System Performance Bank 2 | ECM | DTC P0008 or P0009
P0010 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0011 | Intake Camshaft Position (CMP) System Performance Bank 1 | ECM | DTC P0011, P0014, P0021, or P0024
P0013 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0014 | Exhaust Camshaft Position (CMP) System Performance Bank 1 | ECM | DTC P0011, P0014, P0021, or P0024
P0016 | Crankshaft/Camshaft Correlation | ECM | DTC P0016, P0340, or P0341 for the 2.0L engine
Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019 for the 2.8L, 3.2L, or 3.6L engine
P0017 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019
P0018 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019
P0019 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019
P0020 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0021 | Intake Camshaft Position (CMP) System Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0023 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0024 | Exhaust Camshaft Position (CMP) System Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0030 | HO2S Heater Control Circuit Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.4L engine or DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.2L, or 3.6L engine
P0031 | HO2S Heater Control Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.4L engine or DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.2L, or 3.6L engine
P0032 | HO2S Heater Control Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.4L engine or DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.2L, or 3.6L engine
P0036 | HO2S Heater Control Circuit Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.4L engine or DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.2L, or 3.6L engine
P0037 | HO2S Heater Control Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.4L engine or DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.2L, or 3.6L engine
P0038 | HO2S Heater Control Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.4L engine or DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.2L, or 3.6L engine
P0045 | Boost Pressure Valve | ECM | DTC P0045, P0047, or P0048
P0047 |  | ECM | DTC P0045, P0047, or P0048
P0048 |  | ECM | DTC P0045, P0047, or P0048
P0050 | HO2S Heater Control Circuit Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0051 | HO2S Heater Control Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0052 | HO2S Heater Control Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0053 | HO2S Heater Resistance Bank 1 Sensor 1 | ECM | DTC P0053 or P0059
P0056 | HO2S Heater Control Circuit Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0057 | HO2S Heater Control Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0058 | HO2S Heater Control Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0059 | HO2S Heater Resistance Bank 2 Sensor 1 | ECM | DTC P0053 or P0059
P0069 | Atmospheric Pressure Not Plausible With Boost Pressure | ECM | DTC P0069
P0087 | Rail Pressure | ECM | DTC P0087, P0088, or P0089
P0088 | Rail Pressure High Pressure | ECM | DTC P0087, P0088, or P0089
P0089 | Fuel Metering Solenoid Valve Circuit Range/Performance | ECM | DTC P0087, P0088, or P0089
P0090 | Fuel Metering Solenoid Valve | ECM | DTC P0090, P0091, or P0092
P0091 |  | ECM | DTC P0090, P0091, or P0092
P0092 |  | ECM | DTC P0090, P0091, or P0092
P0095 | Charge Air Temperature Sensor | ECM | DTC P0095, P0097, or P0098
P0097 |  | ECM | DTC P0095, P0097, or P0098
P0098 |  | ECM | DTC P0095, P0097, or P0098
P0100 | Mass or Volume Air Flow Circuit | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L engine
Mass Air Flow (MAF) Sensor Circuit | ECM | DTC P0100, P0102, or P0103 for the 2.8L, 3.2L, or 3.6L engine
P0101 | Airmass Ratio is Higher Than Threshold High | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L engine
Mass Air Flow (MAF) Sensor Performance | ECM | DTC P0101 for the 2.8L, 3.2L, or 3.6L engine
P0102 | Mass Air Flow (MAF) Sensor Circuit Low Frequency | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L engine or DTC P0100, P0102, or P0103 for the 2.8L, 3.2L, or 3.6L engine
P0103 | Mass Air Flow (MAF) Sensor Circuit High Frequency | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L engine or DTC P0100, P0102, or P0103 for the 2.8L, 3.2L, or 3.6L engine
P0105 | Boost Pressure Sensor Circuit | ECM | DTC P0105, P0107, or P0108
P0106 |  | ECM | DTC P0106
P0107 |  | ECM | DTC P0105, P0107, or P0108 for the 2.0L engine or DTC P0107 or P0108 for the 2.4L engine
P0108 |  | ECM | DTC P0105, P0107, or P0108 for the 2.0L engine or DTC P0107 or P0108 for the 2.4L engine
P0110 |  | ECM | DTC P0110
P0111 | Intake Air Temperature (IAT) Sensor Performance | ECM | DTC P0111-P0113
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM | DTC P0112 or P0113 for the 2.4L engine or DTC P0111-P0113 for the 2.8L, 3.2L, or 3.6L engine
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM | DTC P0112 or P0113 for the 2.4L engine or DTC P0111-P0113 for the 2.8L, 3.2L, or 3.6L engine
P0115 | Coolant Temperature Sensor Circuit | ECM | DTC P0115, P0116, P0117, or P0118
P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM |

• | DTC P0115, P0116, P0117, or P0118 for the 2.0L engine

• | DTC P0116 for the 2.4L engine

• | DTC P0116 for the 2.8L, 3.2L, or 3.6L engine

P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM |

• | DTC P0115, P0116, P0117, or P0118 for the 2.0L engine

• | DTC P0117 or P0118 for the 2.4L engine

• | DTC P0117 or P0118 for the 2.8L, 3.2L, or 3.6L engine

P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM |

• | DTC P0115, P0116, P0117, or P0118 for the 2.0L engine

• | DTC P0117 or P0118 for the 2.4L engine

• | DTC P0117 or P0118 for the 2.8L, 3.2L, or 3.6L engine

P0119 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent | ECM | DTC P0119
P0121 | Throttle Position (TP) Sensor 1 Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135 for the 2.4L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.2L, or 3.6L engine
P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135 for the 2.4L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.2L, or 3.6L engine
P0123 | Throttle Position (TP) Sensor 1 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135 for the 2.4L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.2L, or 3.6L engine
P0125 | Engine Coolant Temperature (ECT) Insufficient for Closed Loop Fuel Control | ECM | DTC P0125 for the 2.4L engine or DTC P0125 or P0128 for the 2.8L, 3.2L, or 3.6L engine
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0125 or P0128
P0130 | HO2S Circuit Closed Loop (CL) Performance Bank 1 Sensor 1 | ECM | DTC P0130 or P0150
P0131 | HO2S Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.4L engine or DTC P0131 or P0151 for the 2.8L, 3.2L, or 3.6L engine
P0132 | HO2S Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.4L engine or DTC P0132 or P0152 for the 2.8L, 3.2L, or 3.6L engine
P0133 | HO2S Slow Response Bank 1 Sensor 1 | ECM | DTC P0133 for the 2.4L engine or DTC P0133 or P0153 for the 2.8L, 3.2L, or 3.6L engine
P0134 |  | ECM | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.4L engine or DTC P0134 or P0154 for the 2.8L, 3.2L, or 3.6L engine
P0135 | HO2S Heater Performance Bank 1 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161
P0137 | HO2S Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.4L engine or DTC P0137, P0138, P0140, P0157, P0158, or P0160 for the 2.8L, 3.2L, or 3.6L engine
P0138 | HO2S Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.4L engine or DTC P0137, P0138, P0140, P0157, P0158, or P0160 for the 2.8L, 3.2L, or 3.6L engine
P0140 | HO2S Circuit Insufficient Activity Bank 1 Sensor 2 | ECM | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.4L engine or DTC P0137, P0138, P0140, P0157, P0158, or P0160 for the 2.8L, 3.2L, or 3.6L engine
P0141 | HO2S Heater Performance Bank 1 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161
P0150 | HO2S Circuit Closed Loop (CL) Performance Bank 2 Sensor 1 | ECM | DTC P0130 or P0150
P0151 | HO2S Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0131 or P0151
P0152 | HO2S Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0132 or P0152
P0153 | HO2S Slow Response Bank 2 Sensor 1 | ECM | DTC P0133 or P0153
P0154 |  | ECM | DTC P0134 or P0154
P0155 | HO2S Heater Performance Bank 2 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161
P0157 | HO2S Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0158 | HO2S Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0159 | HO2S Slow Response Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0160 | HO2S Circuit Insufficient Activity Bank 1 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0161 | HO2S Heater Performance Bank 2 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161
P0180 | Fuel Temperature Sensor Circuit | ECM | DTC P0180, P0182, or P0183
P0182 |  | ECM | DTC P0180, P0182, or P0183
P0183 |  | ECM | DTC P0180, P0182, or P0183
P0190 |  | ECM | DTC P0190, P0191, P0192, or P0193
P0191 | Rail Pressure Range/Performance | ECM | DTC P0190, P0191, P0192, or P0193
P0192 |  | ECM | DTC P0190, P0191, P0192, or P0193
P0193 |  | ECM | DTC P0190, P0191, P0192, or P0193
P0201 | No Load Error | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L engine
Injector 1 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0202 | No Load Error | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L engine
Injector 2 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0203 | No Load Error | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L engine
Injector 3 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0204 | Cylinder 4 Injector Circuit Open | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L engine
Injector 4 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0205 | Injector 5 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0206 | Injector 6 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0219 | Engine Overspeed | ECM | DTC P0219
P0221 | Throttle Position (TP) Sensor 2 Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135 for the 2.4L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.2L, or 3.6L engine
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135 for the 2.4L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.2L, or 3.6L engine
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135 for the 2.4L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.2L, or 3.6L engine
P0234 | Boost Pressure Control Circuit Negative Deviation | ECM | DTC P0234 or P0299
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0263 | Cylinder 1 Balance System | ECM | DTC P0263, P0266, P0269, or P0272
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0266 | Cylinder 2 Balance System | ECM | DTC P0263, P0266, P0269, or P0272
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0269 | Cylinder 3 Balance System | ECM | DTC P0263, P0266, P0269, or P0272
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0272 | Cylinder 4 Balance System | ECM | DTC P0263, P0266, P0269, or P0272
P0273 | Injector 5 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0274 | Injector 5 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0276 | Injector 6 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0277 | Injector 6 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0299 | Boost Pressure Control Circuit Positive Deviation | ECM | DTC P0234 or P0299
P02E0 | Electronic Throttle Control | ECM | DTC P02E0, P02E2, or P02E3
P02E1 | Diesel Intake Airflow Performance During Regeneration | ECM | DTC P02E1
P02E2 |  | ECM | DTC P02E0, P02E2, or P02E3
P02E3 |  | ECM | DTC P02E0, P02E2, or P02E3
P0300 | Engine Misfire Detected | ECM | DTC P0300-P0304 for the 2.4L engine or DTC P0300-P0306 for the 2.8L, 3.2L, or 3.6L engine
P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0300-P0304 for the 2.4L engine or DTC P0300-P0306 for the 2.8L, 3.2L, or 3.6L engine
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0300-P0304 for the 2.4L engine or DTC P0300-P0306 for the 2.8L, 3.2L, or 3.6L engine
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0300-P0304 for the 2.4L engine or DTC P0300-P0306 for the 2.8L, 3.2L, or 3.6L engine
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0300-P0304 for the 2.4L engine or DTC P0300-P0306 for the 2.8L, 3.2L, or 3.6L engine
P0305 | Cylinder 5 Misfire Detected | ECM | DTC P0300-P0306
P0306 | Cylinder 6 Misfire Detected | ECM | DTC P0300-P0306
P0313 | Misfire Detected With Low Fuel Level | ECM | DTC P0313
P0318 |  | ECM | DTC P0318
P0324 | Knock Sensor (KS) Module Performance | ECM | DTC P0324 for the 2.4L engine or DTC P0324 for the 2.8L, 3.2L, or 3.6L engine
P0327 | Knock Sensor (KS) Circuit Low Voltage Bank 1 | ECM | DTC P0327 or P0328 for the 2.4L engine or DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.2L, or 3.6L engine
P0328 | Knock Sensor (KS) Circuit High Voltage Bank 1 | ECM | DTC P0327 or P0328 for the 2.4L engine or DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.2L, or 3.6L engine
P0332 | Knock Sensor (KS) Circuit Low Voltage Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0333 | Knock Sensor (KS) Circuit High Voltage Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0335 | Crankshaft Failure No Crankshaft Signal | ECM | DTC P0335 or P0336 for the 2.0L engine
Crankshaft Position (CKP) Sensor Circuit | ECM | DTC P0335, P0336, P0337, or P0338 for the 2.4L engine or DTC P0335, P0336, or P0338 for the 2.8L, 3.2L, or 3.6L engine
P0336 | Crankshaft Position (CKP) Sensor Performance | ECM |

• | DTC P0335 or P0336 for the 2.0L engine

• | DTC P0335, P0336, P0337, or P0338 for the 2.4L engine

• | DTC P0335, P0336, or P0338 for the 2.8L, 3.2L, or 3.6L engine

P0337 | Crankshaft Position (CKP) Sensor Circuit Duty Low Cycle | ECM | DTC P0335, P0336, P0337, or P0338 for the 2.4L engine
P0338 | Crankshaft Position (CKP) Sensor Circuit Duty High Cycle | ECM | DTC P0335, P0336, P0337, or P0338 for the 2.4L engine or DTC P0335, P0336, or P0338 for the 2.8L, 3.2L, or 3.6L engine
P0340 | Camshaft Failure | ECM | DTC P0016, P0340, or P0341 for the 2.0L engine
Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0340, P0341, P0342, or P0343 for the 2.4L engine
P0341 | Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0016, P0340, or P0341 for the 2.0L engine
Intake Camshaft Position (CMP) Sensor Performance Bank 1 | ECM | DTC P0340, P0341, P0342, or P0343 for the 2.4L engine
P0342 | Intake Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 1 | ECM | DTC P0340, P0341, P0342, or P0343
P0343 | Intake Camshaft Position (CMP) Sensor Circuit High Voltage Bank 1 | ECM | DTC P0340, P0341, P0342, or P0343
P0350 | Ignition Coil Control Circuit | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0351 | Ignition 1 Coil Control Circuit | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0352 | Ignition 2 Coil Control Circuit | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0353 | Ignition 3 Coil Control Circuit | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0354 | Ignition 4 Coil Control Circuit | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0355 | Ignition 5 Coil Control Circuit | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0356 | Ignition 6 Coil Control Circuit | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0401 |  | ECM | DTC P0401 or P0402
P0402 |  | ECM | DTC P0401 or P0402
P0403 | Exhaust Gas Recirculation | ECM | DTC P0403, P0489, or P0490 for the 2.0L engine
| ECM | DTC P0403, P0489, or P0490 for the 2.4L engine
P0404 |  | ECM | DTC P0404, P0405, P0406, P046C, or P049D
P0405 |  | ECM | DTC P0404, P0405, P0406, P046C, or P049D
P0406 |  | ECM | DTC P0404, P0405, P0406, P046C, or P049D
P0420 | Catalyst System Low Efficiency Bank 1 | ECM | DTC P0420 for the 2.4L engine or DTC P0420 or P0430 for the 2.8L, 3.2L, or 3.6L engine
P0430 | Catalyst System Low Efficiency Bank 2 | ECM | DTC P0420 or P0430
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM | DTC P0443, P0458, or P0459 for the 2.4L engine or DTC P0443, P0458, or P0459 for the 2.8L, 3.2L, or 3.6L engine
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0443, P0458, or P0459 for the 2.4L engine or DTC P0443, P0458, or P0459 for the 2.8L, 3.2L, or 3.6L engine
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit High Voltage | ECM | DTC P0443, P0458, or P0459 for the 2.4L engine or DTC P0443, P0458, or P0459 for the 2.8L, 3.2L, or 3.6L engine
P0461 | Fuel Level Sensor 1 Performance | ECM | DTC P0461
P0462 | Fuel Level Sensor 1 Circuit Low Voltage | ECM | DTC P0462
P0463 | Fuel Level Sensor 1 Circuit High Voltage | ECM | DTC P0463
P046C |  | ECM | DTC P0404, P0405, P0406, P046C, or P049D
P0480 | Cooling Fan Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0481 | Cooling Fan Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0489 |  | ECM | DTC P0403, P0489, or P0490 for the 2.0L engine or DTC P0403, P0489, or P0490 for the 2.4L engine
P0490 |  | ECM | DTC P0403, P0489, or P0490 for the 2.0L engine or DTC P0403, P0489, or P0490 for the 2.4L engine
P049D |  | ECM | DTC P0404, P0405, P0406, P046C, or P049D
P0500 | Vehicle Speed Signal | ECM | DTC P0500, P0502, or P0503
P0502 |  | ECM | DTC P0500, P0502, or P0503
P0503 |  | ECM | DTC P0500, P0502, or P0503
P0506 | Idle Speed Low | ECM | DTC P0506 or P0507 for the 2.4L engine or DTC P0506 or P0507 for the 2.8L, 3.2L, or 3.6L engine
P0507 | Idle Speed High | ECM | DTC P0506 or P0507 for the 2.4L engine or DTC P0506 or P0507 for the 2.8L, 3.2L, or 3.6L engine
P0513 | Theft Deterrent Key Incorrect | ECM | DTC P0513
P0520 | Engine Oil Pressure (EOP) Switch Circuit | ECM | DTC P0520
P0532 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 or P0533
P0533 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit High Voltage | ECM | DTC P0532 or P0533
P0544 | Exhaust Gas Temperature Sensor | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033
P0545 |  | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033
P0546 |  | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033
P0562 | System Voltage Low | TCM | DTC P0562
P0563 | System Voltage High | TCM | DTC P0563
P0571 | Cruise Control Brake Switch Circuit | ECM | DTC P0571
P0601 |  | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine
Control Module Read Only Memory (ROM) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601
P0602 | Vehicle Coding Is Not Programmed | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine
Control Module Not Programmed | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
Transmission Control Module (TCM) Not Programmed | TCM | DTC P0602
P0603 |  | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine
| ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
Transmission Control Module (TCM) Long Term Memory Reset | TCM | DTC P0603
P0604 |  | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine
Control Module Random Access Memory (RAM) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
Transmission Control Module (TCM) Random Access Memory (RAM) | TCM | DTC P0604
P0605 |  | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine

P0606 | Electronic Control Unit (ECU) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine
Control Module Internal Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
P0607 | Replace Electronic Control Unit (ECU) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine
| ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
P060A | Internal Supply Voltage Upper Limit | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P060B |  | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P0615 | Starter Relay Control Circuit | ECM | DTC P0615
P0616 | Starter Relay Control Circuit Low Voltage | ECM | DTC P0616
P0617 | Starter Relay Control Circuit High Voltage | ECM | DTC P0617
P061C | Electronic Control Unit (ECU) Malfunction | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P0621 | Generator 1 L-Terminal Circuit | ECM | DTC P0621
P0625 | Generator F-Terminal Low Voltage | ECM | DTC P0625
P0626 | Generator F-Terminal High Voltage | ECM | DTC P0626
P0627 | Fuel Pump Primary Circuit | ECM | DTC P0627 for the 2.0L engine
Fuel Pump Relay Control Circuit Open | ECM | DTC P0627, P0628, or P0629 for the 2.4L engine or DTC P0627, P0628, or P0629 for the 2.8L, 3.2L, or 3.6L engine
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0627, P0628, or P0629 for the 2.4L engine or DTC P0627, P0628, or P0629 for the 2.8L, 3.2L, or 3.6L engine
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0627, P0628, or P0629 for the 2.4L engine or DTC P0627, P0628, or P0629 for the 2.8L, 3.2L, or 3.6L engine
P062B | Replace Electronic Control Unit (ECU) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P062F | Electrically Erasable Programmable Read-Only Memory (EEPROM) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P0630 |  | ECM | DTC P0630 for the 2.0L engine or DTC P0630 for the 2.4L engine
P0633 | Theft Deterrent Key Not Programmed - ECM/ECM | ECM | DTC P0633
P0638 | Throttle Actuator Control (TAC) Command Performance | ECM | DTC P0638, P2100, P2101, or P2119 for the 2.4L engine or DTC P0638, P2100, P2101, or P2119 for the 2.8L, 3.2L, or 3.6L engine
P0641 | 5-Volt Reference 1 Circuit | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0642 | 5-Volt Reference 1 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0643 | 5-Volt Reference 1 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0645 | Air Conditioning (A/C) Clutch Relay Control Circuit | ECM | DTC P0645, P0646, or P0647
P0646 | Air Conditioning (A/C) Clutch Relay Control Circuit Low Voltage | ECM | DTC P0645, P0646, or P0647
P0647 | Air Conditioning (A/C) Clutch Relay Control Circuit High Voltage | ECM | DTC P0645, P0646, or P0647
P064C | Glow Plug Module Control Circuit | ECM | DTC P064C
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650
P0651 | 5-Volt Reference 2 Circuit | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0652 | 5-Volt Reference 2 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0653 | 5-Volt Reference 2 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0670 | PWM-Actuator | ECM | DTC P0670
P0671 | Cylinder 1 Glow Plug Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0672 | Cylinder 2 Glow Plug Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0673 | Cylinder 3 Glow Plug Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0674 | Cylinder 4 Glow Plug Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0683 | Glow Plug | ECM | DTC P0683
P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0686 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0687 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0689 | Engine Controls Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0689 for the 2.4L engine or DTC P0685, P0686, P0687, P0689, or P0690 for the 2.8L, 3.2L, or 3.6L engine
P068A |  | ECM | DTC P068A, P068B, or P2510
P068B |  | ECM | DTC P068A, P068B, or P2510
P0690 | Engine Controls Ignition Relay Feedback Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0691 | Cooling Fan Relay 1 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0692 | Cooling Fan Relay 1 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0693 | Cooling Fan Relays 2 and 3 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0694 | Cooling Fan Relays 2 and 3 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0697 | 5-Volt Reference 3 Circuit | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0698 | 5-Volt Reference 3 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0699 | 5-Volt Reference 3 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM |

• | DTC P0700 for the 2.0L engine

• | DTC P0700 for the 2.4L engine

• | DTC P0700 for the 2.8L, 3.2L, or 3.6L engine

P0703 | Brake Switch Circuit | TCM | DTC P0703
P0705 | Transmission Range (TR) Switch Circuit | TCM | DTC P0705
P0711 | Transmission Fluid Temperature (TFT) Sensor Performance | TCM | DTC P0711
P0712 | Transmission Fluid Temperature (TFT) Sensor Circuit Low Voltage | TCM | DTC P0712
P0713 | Transmission Fluid Temperature (TFT) Sensor Circuit High Voltage | TCM | DTC P0713
P0717 | Input Speed Sensor Circuit Low Voltage | TCM | DTC P0717
P0722 | Output Speed Sensor Circuit Low Voltage | TCM | DTC P0722
P0727 | Engine Speed Signal | TCM | DTC P0727
P0730 | Incorrect Gear Ratio | TCM | DTC P0730
P0731 | Incorrect 1st Gear Ratio | TCM | DTC P0731
P0732 | Incorrect 2nd Gear Ratio | TCM | DTC P0732
P0733 | Incorrect 3rd Gear Ratio | TCM | DTC P0733
P0734 | Incorrect 4th Gear Ratio | TCM | DTC P0734
P0735 | Incorrect 5th Gear Ratio | TCM | DTC P0735
P0736 | Incorrect Reverse Gear Ratio | TCM | DTC P0736
P0741 | Torque Converter Clutch (TCC) System - Stuck OFF | TCM | DTC P0741
P0742 | Torque Converter Clutch (TCC) System - Stuck ON | TCM | DTC P0742
P0762 | 4-5 Shift Solenoid (SS) Performance - No Fifth Gear | TCM | DTC P0762
P0800 | Active Transfer Case (ATC) Control Module Requested MIL Illumination | ECM | DTC P0800 for the 2.0L engine or DTC P0800 for the 2.4L engine
P0856 | ABS Torque Signal Malfunction | ECM | DTC P0856
P0897 | Transmission Fluid Life | TCM | DTC P0897
P0962 | Line Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0962
P0963 | Line Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0963
P0966 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0966
P0967 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0967
P0970 | Shift Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0970
P0971 | Shift Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0971
P0973 | Shift Solenoid (SS) 1 Control Circuit Low Voltage | TCM | DTC P0973
P0974 | Shift Solenoid (SS) 1 Control Circuit High Voltage | TCM | DTC P0974
P0976 | Shift Solenoid (SS) 2 Control Circuit Low Voltage | TCM | DTC P0976
P0977 | Shift Solenoid (SS) 2 Control Circuit High Voltage | TCM | DTC P0977
P0979 | Shift Solenoid (SS) 3 Control Circuit Low Voltage | TCM | DTC P0979
P0980 | Shift Solenoid (SS) 3 Control Circuit High Voltage | TCM | DTC P0980
P0982 | Shift Solenoid (SS) 4 Control Circuit Low Voltage | TCM | DTC P0982
P0983 | Shift Solenoid (SS) 4 Control Circuit High Voltage | TCM | DTC P0983
P0985 | Shift Solenoid (SS) 5 Control Circuit Low Voltage | TCM | DTC P0985
P0986 | Shift Solenoid (SS) 5 Control Circuit High Voltage | TCM | DTC P0986
P1011 | Intake Camshaft Position (CMP) Actuator Park Position Bank 1 | ECM | DTC P1011-P1014
P1012 | Exhaust Camshaft Position (CMP) Actuator Park Position Bank 1 | ECM | DTC P1011-P1014
P1013 | Intake Camshaft Position (CMP) Actuator Park Position Bank 2 | ECM | DTC P1011-P1014
P1014 | Exhaust Camshaft Position (CMP) Actuator Park Position Bank 2 | ECM | DTC P1011-P1014
P1138 |  | ECM | DTC P1138
P1224 |  | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233
P1227 |  | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233
P122A |  | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233
P1233 |  | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233
P1446 |  | ECM | DTC P1446, P1447, P244C, or P244D
P1447 | Pre-catalyst Temperature Too High During Regeneration | ECM | DTC P1446, P1447, P244C, or P244D
P1551 | Throttle Valve Rest Position Not Reached During Learn | ECM | DTC P1551 for the 2.4L engine or DTC P1551 for the 2.8L, 3.2L, or 3.6L engine
P1600 |  | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
P161C | Tire Circumference Not Programmed | ECM | DTC P161C
P161E | Glow Plug Module Control Circuit | ECM | DTC P161E
P161F |  | ECM | DTC P161F
P1621 |  | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
P1627 |  | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
P1629 | Theft Deterrent Start Enable Signal Not Received | ECM | DTC P1629
P1631 | Theft Deterrent Start Enable Signal Not Correct | ECM | DTC P1631
P1632 | Theft Deterrent Start Disable Signal Received | ECM | DTC P1632
P1668 | Generator L-Terminal Control Circuit | ECM | DTC P1668
P1680 |  | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
P1681 |  | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
P1682 |  | ECM | DTC P1682
P1683 |  | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
P1715 |  | TCM | DTC P1715
P1719 | Incorrect Shifting Detected | TCM | DTC P1719
P1845 |  | ECM | DTC P1845
P2002 | Particulate Trap Efficiency Below Threshold Bank 1 | ECM | DTC P2002
P2008 | Intake Manifold Runner Control (IMRC) Solenoid Control Circuit | ECM | DTC P2008, P2009, or P2010
P2009 | Intake Manifold Runner Control (IMRC) Solenoid Control Circuit Low Voltage | ECM | DTC P2008, P2009, or P2010
P2010 | Intake Manifold Runner Control (IMRC) Solenoid Control Circuit High Voltage | ECM | DTC P2008, P2009, or P2010
P2031 | Catalyst Temperature Sensor Circuit Bank 1 Sensor 2 | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033
P2032 |  | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033
P2033 |  | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033
P2066 | Fuel Level Sensor 2 Performance | ECM | DTC P2066
P2067 | Fuel Level Sensor 2 Circuit Low Voltage | ECM | DTC P2067
P2068 | Fuel Level Sensor 2 Circuit High Voltage | ECM | DTC P2068
P2080 | Catalyst Temperature Sensor Range/Performance Bank 1 | ECM | DTC P2080 or P2084
P2084 | Catalyst Temperature Sensor Performance Bank 1 Sensor 2 | ECM | DTC P2080 or P2084
P2088 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2089 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2090 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2091 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2092 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2093 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2094 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2095 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2096 | Post Catalyst Fuel Trim System Low Limit Bank 1 | ECM | DTC P2096 for the 2.4L engine or DTC P2096 or P2098 for the 2.8L, 3.2L, or 3.6L engine
P2097 | Post Catalyst Fuel Trim System High Limit Bank 1 | ECM | DTC P2097 for the 2.4L engine or DTC P2097 or P2099 for the 2.8L, 3.2L, or 3.6L engine
P2098 | Post Catalyst Fuel Trim System Low Limit Bank 2 | ECM | DTC P2096 or P2098
P2099 | Post Catalyst Fuel Trim System High Limit Bank 2 | ECM | DTC P2097 or P2099
P20E2 | Catalyst Temperature Sensor Range/Performance Bank 1 | ECM | DTC P20E2
P2100 | Throttle Actuator Control (TAC) Motor Control Circuit | ECM | DTC P0638, P2100, P2101, or P2119 for the 2.4L engine or DTC P0638, P2100, P2101, or P2119 for the 2.8L, 3.2L, or 3.6L engine
P2101 | Control Module Throttle Actuator Position Performance | ECM | DTC P0638, P2100, P2101, or P2119 for the 2.4L engine or DTC P0638, P2100, P2101, or P2119 for the 2.8L, 3.2L, or 3.6L engine
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shutdown | ECM | DTC P2105
P2107 | Throttle Actuator Control (TAC) Module Internal Circuit | ECM | DTC P2107 for the 2.4L engine or DTC P2107 for the 2.8L, 3.2L, or 3.6L engine
P2111 | Throttle Actuator Control (TAC) Throttle Valve Stuck Open | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2119 | Throttle Closed Position Performance | ECM | DTC P0638, P2100, P2101, or P2119 for the 2.4L engine or DTC P0638, P2100, P2101, or P2119 for the 2.8L, 3.2L, or 3.6L engine
P2120 | Accelerator Pedal Position (APP) Sensor 1 | ECM | DTC P2120, P2125, or P2138
P2121 |  | ECM | DTC P2121, P2122, P2123, P2127, P2128, or P2138
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2121, P2122, P2123, P2127, P2128, or P2138 for the 2.4L engine or DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.2L, or 3.6L engine
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2121, P2122, P2123, P2127, P2128, or P2138 for the 2.4L engine or DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.2L, or 3.6L engine
P2125 | Accelerator Pedal Position (APP) Sensor 2 |  | DTC P2120, P2125, or P2138
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2121, P2122, P2123, P2127, P2128, or P2138 for the 2.4L engine or DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.2L, or 3.6L engine
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2121, P2122, P2123, P2127, P2128, or P2138 for the 2.4L engine or DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.2L, or 3.6L engine
P2135 |  | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135
P2138 | Accelerator Pedal Position (APP) Sensor 1 and 2 Signal Incorrect Ratio | ECM | DTC P2120, P2125, or P2138 for the 2.0L engine
Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2121, P2122, P2123, P2127, P2128, or P2138 for the 2.4L engine or DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.2L, or 3.6L engine
P2146 | Injector 1 or 4 | ECM | DTC P2146 or P2149
P2149 | Injector 2 or 3 | ECM | DTC P2146 or P2149
P2176 | Minimum Throttle Position Not Learned | ECM | DTC P2176 for the 2.4L engine or DTC P2176 for the 2.8L, 3.2L, or 3.6L engine
P2177 | Fuel Trim System Lean at Cruise or Accel Bank 1 | ECM | DTC P2177, P2187, or P2191 for the 2.4L engine or DTC P2177, P2179, P2187, or P2189 for the 2.8L, 3.2L, or 3.6L engine
P2178 | Fuel Trim System Rich at Cruise or Accel Bank 1 | ECM | DTC P2178, P2188, or P2192 for the 2.4L engine or DTC P2178, P2180, P2188, or P2190 for the 2.8L, 3.2L, or 3.6L engine
P2179 | Fuel Trim System Lean at Cruise or Accel Bank 2 | ECM | DTC P2177, P2179, P2187, or P2189
P2180 | Fuel Trim System Rich at Cruise or Accel Bank 2 | ECM | DTC P2178, P2180, P2188, or P2190
P2187 | Fuel Trim System Lean at Idle Bank 1 | ECM | DTC P2177, P2187, or P2191 for the 2.4L engine or DTC P2177, P2179, P2187, or P2189 for the 2.8L, 3.2L, or 3.6L engine
P2188 | Fuel Trim System Rich at Idle Bank 1 | ECM | DTC P2178, P2188, or P2192 for the 2.4L engine or DTC P2178, P2180, P2188, or P2190 for the 2.8L, 3.2L, or 3.6L engine
P2189 | Fuel Trim System Lean at Idle Bank 2 | ECM | DTC P2177, P2179, P2187, or P2189
P2190 | Fuel Trim System Rich at Idle Bank 2 | ECM | DTC P2178, P2180, P2188, or P2190
P2191 |  |  | DTC P2177, P2187, or P2191
P2192 |  |  | DTC P2178, P2188, or P2192
P2195 | HO2S Signal Biased Lean Bank 1 Sensor 1 | ECM | DTC P2195 or P2197
P2196 | HO2S Signal Biased Rich Bank 1 Sensor 1 | ECM | DTC P2196 or P2198
P2197 | HO2S Signal Biased Lean Bank 2 Sensor 1 | ECM | DTC P2195 or P2197
P2198 | HO2S Signal Biased Rich Bank 2 Sensor 1 | ECM | DTC P2196 or P2198
P2226 |  | ECM | DTC P2226, P2228, or P2229
P2227 | Barometric Pressure (BARO) Sensor Performance | ECM | DTC P2227, P2228, or P2229
P2228 | Barometric Pressure (BARO) Sensor Circuit Low Voltage | ECM | DTC P2226, P2228, or P2229 for the 2.0L engine or DTC P2227, P2228, or P2229 for the 2.8L, 3.2L, or 3.6L engine
P2229 | Barometric Pressure (BARO) Sensor Circuit High Voltage | ECM | DTC P2226, P2228, or P2229 for the 2.0L engine or DTC P2227, P2228, or P2229 for the 2.8L, 3.2L, or 3.6L engine
P2231 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 1 | ECM | DTC P2231 or 2232 for the 2.4L engine or DTC P2231 or P2234 for the 2.8L, 3.2L, or 3.6L engine
P2232 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 2 | ECM | DTC P2231 or 2232 for the 2.4L engine or DTC P2232 or P2235 for the 2.8L, 3.2L, or 3.6L engine
P2234 | HO2S Signal Circuit Shorted to Heater Circuit Bank 2 Sensor 1 | ECM | DTC P2231 or P2234
P2235 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 2 | ECM | DTC P2232 or P2235
P2264 | Fuel Filter Water Level Sensing Sensor Self-test Signal Error | ECM | DTC P2264
P2270 | HO2S Signal Stuck Lean Bank 1 Sensor 2 | ECM | DTC P2270 for the 2.4L engine or DTC P2270 or P2272 for the 2.8L, 3.2L, or 3.6L engine
P2271 | HO2S Signal Stuck Rich Bank 1 Sensor 2 | ECM | DTC P2271 for the 2.4L engine or DTC P2271 or P2273 for the 2.8L, 3.2L, or 3.6L engine
P2272 | HO2S Signal Stuck Lean Bank 2 Sensor 2 | ECM | DTC P2270 or P2272
P2273 | HO2S Signal Stuck Rich Bank 2 Sensor 2 | ECM | DTC P2271 or P2273
P2293 | Rail Pressure | ECM | DTC P2293, P2294, P2295, or P2296
P2294 | Rail Pressure Control Solenoid Valve Circuit | ECM | DTC P2293, P2294, P2295, or P2296
P2295 |  | ECM | DTC P2293, P2294, P2295, or P2296
P2296 |  | ECM | DTC P2293, P2294, P2295, or P2296
P2297 | HO2S Performance During Decel Fuel Cut-Off (DFCO) Bank 1 Sensor 1 | ECM | DTC P2297 or P2298
P2298 | HO2S Performance During Decel Fuel Cut-Off (DFCO) Bank 2 Sensor 1 | ECM | DTC P2297 or P2298
P2299 | Accelerator Pedal and Brake Plausibility | ECM | DTC P2299
P2300 | Ignition Coil 1 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2301 | Ignition Coil 1 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2303 | Ignition Coil 2 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2304 | Ignition Coil 2 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2306 | Ignition Coil 3 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2307 | Ignition Coil 3 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2309 | Ignition Coil 4 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2310 | Ignition Coil 4 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2312 | Ignition Coil 5 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2313 | Ignition Coil 5 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2315 | Ignition Coil 6 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2316 | Ignition Coil 6 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P244A |  | ECM | DTC P244A, P244B, or P2453
P244B | Diesel Particulate Filter Differential Pressure Too High | ECM | DTC P244A, P244B, or P2453
P244C | Catalyst Temperature Too Low During Regeneration | ECM | DTC P1446, P1447, P244C, or P244D
P244D | Catalyst Temperature Too High During Regeneration | ECM | DTC P1446, P1447, P244C, or P244D
P2452 | Diesel Particulate Filter Differential Pressure Sensor Circuit | ECM | DTC P2452, P2454, or P2455
P2453 | Diesel Particulate Filter Differential Pressure Performance | ECM | DTC P244A, P244B, or P2453
P2454 |  | ECM | DTC P2452, P2454, or P2455
P2455 |  | ECM | DTC P2452, P2454, or P2455
P2463 | Diesel Particulate Filter - Soot Accumulation | ECM | DTC P2463
P2500 | Generator L-Terminal Circuit Low Voltage | ECM | DTC P2501
P2501 | Generator L-Terminal Circuit High Voltage | ECM | DTC P2500
P2510 | Main Relay | ECM | DTC P068A, P068B, or P2510
P2533 | Engine Control Module (ECM)/Powertrain Control Module (PCM) Relay Sense Circuit Range/Performance | ECM | DTC P2533
| TCM | DTC P2533
P253F |  | ECM | DTC P253F
P2544 | Invalid Signal From Transmission Control Module (TCM) | ECM | DTC P2544
P2610 |  | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
P2636 | Mechanical Transfer Jet Pump; Fuel Level of Tank 1 Above the Upper Limit and Tank 2 Below the Lower Limit | ECM | DTC P2636 for the 2.0L engine
Fuel Transfer Pump Flow Insufficient | ECM | DTC P2636 for the 2.4L engine
P2687 | Fuel Filter Heater | ECM | DTC P2687
P268A | Injector Quantity Adjustment Not Programmed | ECM | DTC P268A
P2757 |  | TCM | DTC P2757
P2758 |  | TCM | DTC P2758
P2763 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P2763
P2764 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P2764
U0073 | Control Module Communication Bus Off | BCM | DTC U0073
U0100 | Lost Communication With ECM A | BCM | DTC U0100-U0299 or U2105-U2199
U0101 | Lost Communication With TCM | BCM | DTC U0100-U0299 or U2105-U2199
U0102 | Lost Communication With Transfer Case Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0104 | Lost Communication With Cruise Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0121 | Lost Communication With ABS Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0122 | Lost Communication With Vehicle Dynamics Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0131 | Lost Communication With Power Steering Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0132 | Lost Communication With Ride Level Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0134 | Lost Communication With Power Steering Control Module - Rear | BCM | DTC U0100-U0299 or U2105-U2199
U0140 | Lost Communication With Body Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0155 | Lost Communication With Instrument Panel Cluster (IPC) Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0158 | Lost Communication With Head Up Display | BCM | DTC U0100-U0299 or U2105-U2199
U0160 | Lost Communication With Audible Alert Control | BCM | DTC U0100-U0299 or U2105-U2199
U0164 | Lost Communication With Body Control Module (BCM) | BCM | DTC U0100-U0299 or U2105-U2199
U0168 | Lost Communication With Vehicle Security Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0184 | Lost Communication With Radio | BCM | DTC U0100-U0299 or U2105-U2199
U0186 | Lost Communication With Audio Amplifier | BCM | DTC U0100-U0299 or U2105-U2199
U0198 | Lost Communication With Telematic Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0199 | Lost Communication With Door Control Module A | BCM | DTC U0100-U0299 or U2105-U2199
U0200 | Lost Communication With Door Control Module B | BCM | DTC U0100-U0299 or U2105-U2199
U0201 | Lost Communication With Door Control Module C | BCM | DTC U0100-U0299 or U2105-U2199
U0202 | Lost Communication With Door Control Module D | BCM | DTC U0100-U0299 or U2105-U2199
U0214 | Lost Communication With Remote Function Actuation | BCM | DTC U0100-U0299 or U2105-U2199
U0230 | Lost Communication With Rear Gate Module | BCM | DTC U0100-U0299 or U2105-U2199
U0240 | Lost Communication With Headlamp Control Module A | BCM | DTC U0100-U0299 or U2105-U2199
U1814 | Powertrain High Speed Communication Enable Circuit | BCM | DTC U1814
U2099 | High Speed Communication Enable Circuit | BCM | DTC U2099
U2100 | Controller Area Network (CAN) Bus Communication | BCM | DTC U2100
U2101 | Maximum List Of CAN Control Modules Not Programmed | BCM | DTC U2101
U2105 | Lost Communication | BCM | DTC U0100-U0299 or U2105-U2199