For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Maximum Tire and Wheel Assembly Lateral Runout, Off-Vehicle | 1 mm | 0.04 in
Maximum Tire and Wheel Assembly Lateral Runout, On-Vehicle | 0.8 mm | 0.03 in
Maximum Tire and Wheel Assembly Radial Runout Off-Vehicle | 1 mm | 0.04 in
Maximum Tire and Wheel Assembly Radial Runout, On-Vehicle | 0.8 mm | 0.03 in
Maximum Wheel Lateral Runout, Off-Vehicle, Tire Dismounted | 1 mm | 0.04 in
Maximum Wheel Radial Runout, Off-Vehicle, Tire Dismounted | 0.8 mm | 0.03 in
Maximum Wheel Lateral Runout, Off-Vehicle, Tire Mounted | 1 mm | 0.04 in
Maximum Wheel Radial Run out Off-Vehicle, Tire Mounted | 0.8 mm | 0.03 in
Wheel Hub Flange Runout Tolerance Guideline | 0.132 mm | 0.005 in
Wheel Stud Runout Tolerance Guideline | 0.04 mm | 0.002 in