For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the intake air temperature (IAT) sensor connector.
3. Loosen the clamp and disconnect the air cleaner outlet hose from the resonator.
4. Remove the air cleaner housing bolts.
5. Unclip the housing from the ball stud and then remove the air cleaner assembly.

### Installation Procedure

1. Install the air cleaner assembly.
2. Install the air cleaner housing to the ball stud and connect the air cleaner outlet hose to the resonator.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the air cleaner housing bolts.

Tighten
Tighten the air cleaner housing bolts to 6 N·m (53 lb in).