For 1990-2009 cars

### Removal Procedure

1. Siphon the power steering fluid from the fluid reservoir.
2. Remove the reservoir bolts.

Caution: Refer to Power Steering Hose Disconnected Caution in the Preface section.

3. Loosen the hose clamps and remove both hoses from the reservoir.

### Installation Procedure

1. Attach the power steering fluid reservoir to the reservoir bracket.

Caution: Refer to Installing Hoses without Twists or Bends Caution in the Preface section.

2. Connect both hoses to the fluid reservoir and secure the hose clamps.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the fluid reservoir bolts and tighten to 9 N·m (80 lb in).

Caution: Refer to Using Proper Power Steering Fluid Caution in the Preface section.

4. Fill the fluid reservoir with power steering fluid. Refer to Checking and Adding Power Steering Fluid.

Caution: Refer to Air in the Power Steering System Caution in the Preface section.

5. Bleed the system. Refer to Power Steering System Bleeding.
6. Inspect the power steering system for leaks. If there are leaks, correct the cause of the leaks. Refer to Power Steering Fluid Leaks.