For 1990-2009 cars
Battery Voltage Signal 2: The scan tool displays the battery voltage as seen at the liftgate module.
Hall Sensor Feed Status: The scan tool displays No Output/Short to Ground. Than scan tool will display any faults associated with the hall sensor while in motion.
Liftgate Handle Switch Status: The scan tool displays Active/Inactive. The scan tool the status of the liftgate handle switch and the liftgate close switch.
Liftgate Ajar Switch: The scan tool displays Active/Inactive. The scan tool displays the state of the liftgate ajar switch as seen at the rear integration module.
Object Detection Sensor Status: The scan tool displays the voltage as seen through the object sensors.
LGM Clutch Actuator Command: The scan tool displays Active/Inactive. The scan tool displays the commanded state of the liftgate clutch.
LGM Latch Motor Cinch Command: The scan tool displays Active/Inactive. The scan tool displays the commanded state of the cinching portion of the liftgate latch.
LGM Latch Pawl Switch: The scan tool displays Active/Inactive. The scan tool displays the state of the liftgate open switch.
LGM Latch Ratchet Switch: The scan tool displays Active/Inactive. The scan tool displays the state of the liftgate ajar switch.
LGM Motor Release Command: The scan tool displays Active/Inactive. The scan tool displays the commanded state of the release portion of the liftgate latch.
LGM Latch Sector Switch: The scan tool displays Active/Inactive. The scan tool displays the state of the liftgate conch/release switch.
LGM Motor Closed Command: The scan tool displays Active/Inactive. The scan tool displays the commanded state of the liftgate motor during closing.
LGM Motor Open Command: The scan tool displays Active/Inactive. The scan tool displays the commanded state of the liftgate motor during opening.
LGM Open/Close Position Learned: The scan tool displays Yes/No. The scan tool displays the results of the liftgate calibration.
LGM Full Open Switch: The scan tool displays Active/Inactive. The scan tool displays the status of the liftgate full open switch.