For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the quarter window garnish molding. Refer to Body Side Window Rear Garnish Molding Replacement .
3. Disconnect the electrical connector.
4. Remove the bolt and the side glass antenna module.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the side glass antenna module with the bolt.

Tighten
Tighten the side glass antenna module bolt to 8 N·m (11 lb ft).

2. Connect the electrical connectors.
3. Install the quarter window garnish molding. Refer to Body Side Window Rear Garnish Molding Replacement .
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .