For 1990-2009 cars

### Removal Procedure

Warning: Gasoline or gasoline vapors are highly flammable. A fire could occur if an ignition source is present. Never drain or store gasoline or diesel fuel in an open container, due to the possibility of fire or explosion. Have a dry chemical (Class B) fire extinguisher nearby.

1. Disconnect the canister fuel vapor hoses from the canister.
2. Loosen the clamp and disconnect the evaporative emission (EVAP) canister vent hose from the EVAP canister filter
3. Remove the EVAP canister bracket retaining nuts and the EVAP canister assembly.
4. Separate the canister from the EVAP canister bracket.
5. Remove the canister.

### Installation Procedure

1. Install the EVAP canister onto the EVAP canister bracket.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the EVAP canister assembly.

Tighten
Tighten the EVAP canister bracket retaining nuts to 10 N·m (88 lb in).

3. Connect the EVAP canister vent hose to the EVAP canister filter.
4. Connect the canister fuel vapor hoses to the canister.