For 1990-2009 cars

Leak Areas | Repair Materials
--- | ---
Nozzle Type | Full jet spray nozzle #1/2 GG-25 or equivalent with a 60 degree included angle
Nozzle Height | Approximately 1600 mm (63.0 in) from the floor
Volume of Flow | 14 L (3.7 gal) per minute
Pressure | 155 kPa (22.5 psi) measured at the nozzle
Windshield and A-Pillar Test Stand Position | Approximately 30 degrees down, 45 degrees toward the rear, and aimed at the corner of the windshield
B-Pillar Test Stand Position | Approximately 30 degrees down, 45 degrees toward the rear, and aimed at the center of the rear door
Back Window and Rear Deck Lid Test Stand Position | Approximately 30 degrees down, 30 degrees toward the front and aimed approximately 610 mm (24.0 in) from the corner of the back window