For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accessory Drive Belt Idler Pulley Attaching Bolt | 50 N·m | 37 lb ft
Accessory Drive Belt Tensioner Attaching Bolts | 50 N·m | 37 lb ft
Air Cleaner Element Cover Screws | 2 N·m | 18 lb in
Air Cleaner Housing Bolts | 6 N·m | 53 lb in
Battery Hold-Down Bar Bracket Retaining Nuts | 10 N·m | 89 lb in
Battery Tray Retaining Bolts | 10 N·m | 89 lb in
Camshaft Bearing Cap Bolts | 10 N·m | 89 lb in
Camshaft Intermediate Driveshaft Sprocket Attaching Bolt | 65 N·m | 48 lb ft
Camshaft Position Actuator Attaching Bolt | 58 N·m | 43 lb ft
Connecting Rod Cap Bearing Bolts | 35 N·m, Loosen all, 25+110° | 22 lb ft, Loosen all, 18+110°
Coolant Drain Threaded Plug | 31 N·m | 23 lb ft
Cradle Mounting Bolts | 155 N·m | 114 lb ft
Cradle Support Bracket Mounting Bolts | 50 N·m | 37 lb ft
Crankshaft Main Bearing Cap Inboard Attaching Bolt | 20+80° | 15+80°
Crankshaft Main Bearing Cap Outboard Attaching Bolt | 15+110° | 11+110°
Crankshaft Main Bearing Cap Side Attaching Bolt | 30+60° | 22+60°
Crankshaft Oil Deflector Attaching Bolt | 10 N·m | 89 lb in
Crankshaft Pulley Bolts | 100+150° | 74+150°
Crankshaft Rear Oil Seal Housing Attaching Bolt | 10 N·m | 89 lb in
Cylinder Block Rear Oil Gallery Threaded Plug | 31 N·m | 23 lb ft
Cylinder Head Bolts (M11) | 45+120° | 33+120°
Cylinder Head Bolts (M8) | 15+60° | 11+60°
Cylinder Head Cover Bolts | 10 N·m | 89 lb in
Engine Dress Cover Bolts and Nuts | 8 N·m | 71 lb in
Engine Front Cover Assembly Bolts | 23 N·m | 17 lb ft
Engine Fuse Block Lower Cover Bolts | 10 N·m | 89 lb in
Engine Fuse Block Retaining Bolts | 3 N·m | 27 lb in
Engine Lift Bracket Attaching Bolt | 50 N·m | 37 lb ft
Engine Mount Adapter Bolts | 50 N·m | 37 lb ft
Engine Mount Frame Side Bracket Bolt | 100 N·m | 74 lb ft
Engine Mount Frame Side Bracket Nuts | 90 N·m | 66 lb ft
Engine Mount Frame Side Bracket Nuts | 90 N·m | 66 lb-ft
Engine Mount Support Bracket Upper Bolts | 90 N·m | 66 lb ft
Engine Mount Support Bracket Lower Bolt | 50 N·m | 37 lb ft
Evaporative Emission Canister Purge Solenoid Bracket Bolt | 5 N·m | 44 lb in
Exhaust Camshaft Gear Bolt | 50+60°+15° | 37+60°+15°
Exhaust Front Pipe Mounting Bracket Bolt and Nut | 40 N·m | 30 lb ft
Exhaust Manifold Heat Shield Bolts | 10 N·m | 89 lb in
Exhaust Manifold to Cylinder Head Attaching Bolts | 20 N·m | 15 lb ft
Flexible Plate Bolts | 65 N·m | 48 lb ft
Fuel Injector Wiring Harness Bracket Attaching Bolt | 20 N·m | 15 lb ft
Fuel Rail Assembly Retaining Bolts | 25 N·m | 18 lb ft
Fuel Rail Assembly Retaining Bolts | 10 N·m | 89 lb in
Lower Intake Manifold to Cylinder Head Attaching Bolt | 23 N·m | 17 lb ft
Oil Filter Adapter Retaining Bolts | 8 N·m | 71 lb in
Oil Gallery Threaded Plug | 31 N·m | 23 lb ft
Oil Jet Attaching Bolt | 10 N·m | 89 lb in
Oil Level Sensor | 20 N·m | 15 lb ft
Oil Level Stick Gage Tube Attaching Bolt | 10 N·m | 89 lb in
Oil Pan Drain Plug | 25 N·m | 18 lb ft
Oil Pan Flange-to-Transaxle Retaining Bolts | 50 N·m | 37 lb ft
Oil Pan to Crankshaft Rear Oil Seal Housing Attaching Bolt | 10 N·m | 89 lb in
Oil Pan to Cylinder Block Attaching Bolt | 23 N·m | 17 lb ft
Oil Pressure Sensor | 13 N·m | 115 lb in
Oil Pump Retaining Bolts | 23 N·m | 17 lb ft
Oil Suction Pipe Retaining Bolts | 10 N·m | 89 lb in
Primary Timing Chain Tensioner Attaching Bolt | 23 N·m | 17 lb ft
Primary Timing Chain Upper Guide Attaching Bolt | 23 N·m | 17 lb ft
Pup Converter-to-Exhaust Front Pipe Retaining Nuts | 40 N·m | 30 lb ft
Rear Timing Belt Cover Bolts | 7 N·m | 62 lb in
Secondary Timing Chain Guide Attaching Bolt | 23 N·m | 17 lb ft
Secondary Timing Chain Shoe Attaching Bolt | 23 N·m | 17 lb ft
Secondary Timing Chain Tensioner Attaching Bolt | 23 N·m | 17 lb ft
Spark Plugs | 18 N·m | 13 lb ft
Timing Belt Automatic Tensioner Bolt | 25 N·m | 18 lb ft
Timing Belt Idler Pulley Bolt & Nut | 25 N·m | 18 lb ft
Transaxle Front Mount Retaining Bolts | 50 N·m | 37 lb ft
Transaxle Front Mount-to-Transaxle Through Bolt & Nut | 90 N·m | 66 lb ft
Transaxle Mount Assembly Retaining Bolts | 37 N·m | 27 lb ft
Transaxle Mount Bracket Retaining Bolts | 50 N·m | 37 lb ft
Transaxle Rear Mount Bracket Retaining Bolts | 90 N·m | 66 lb ft
Transaxle Rear Mount Retaining Bolts | 90 N·m | 66 lb ft
Transaxle Rear Mount-to-Bracket Through Bolt & Nut | 90 N·m | 66 lb ft
Transaxle-to-Oil Pan Flange Bolt | 50 N·m | 37 lb ft
Transaxle Torque Converter Bolts | 45 N·m | 33 lb ft
Upper Intake Manifold to Cylinder Head Attaching Bolt | 23 N·m | 17 lb ft
Upper Intake Manifold to Lower Intake Manifold Attaching Bolt | 23 N·m | 17 lb ft