For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

Note: Only lift the engine far enough to take the weight off the engine mount assembly.

1. Support the engine assembly using DW-110-060 fixture .
2. Remove the engine mount adapter retaining bolts from the engine mount support bracket.
3. Remove the engine mount frame side bracket retaining bolt and nuts.
4. Remove the engine mount assembly.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the engine mount assembly and tighten.

• | Engine mount frame side bracket retaining bolt to 100 N·m (74 lb ft).

• | Nuts to 90 N·m (66 lb ft).

• | Engine mount adapter retaining bolts to 50 N·m (37 lb ft).

2. Remove the engine assembly support fixture DW-110-060 fixture .