For 1990-2009 cars

Connector 1: | X436 - Object Alarm Module Patch Harness Ground (with GFP)
Connector 2: | X437 - Object Alarm Module Patch Harness (with GFP)

#### X101 Body Harness to Engine Harness

#### Connector Part Information

- OEM: 0-1743059-2
- Service: N/A
- Description: 36-Way F, MTIII/JPT Sealed (BK)

#### Connector Part Information

- OEM: 1743062-2
- Service: N/A
- Description: 36-Way M MTIII/JPT Sealed (BK)

#### X101 Body Harness to Engine Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BU/WH | 6548 | PTC Heater Supply Voltage | 1 | 0.5 BU/WH | 6548 | PTC Heater Supply Voltage
2 | 0.5 WH/BK | 1164 | APM 5-Volt - 1 Reference | 2 | 0.5 WH/BK | 1164 | APM 5-Volt - 1 Reference
3 | 0.5 D-BU | 1161 | APM Sensor 1 Signal | 3 | 0.5 D-BU | 1161 | APM Sensor 1 Signal
4 | 0.5 BN | 1271 | Low Reference | 4 | 0.5 BN | 1271 | Low Reference
5 | 0.5 PU | 1272 | Low Reference | 5 | 0.5 PU | 1272 | Low Reference
6 | 0.5 BK | 1162 | APM Sensor 2 Signal | 6 | 0.5 BK | 1162 | APM Sensor 2 Signal
7 | 0.5 TN | 1274 | 5-Volt Reference | 7 | 0.5 TN | 1274 | 5-Volt Reference
8 | 0.5 PU | 7089 | PTC Supply Voltage | 8 | 0.5 PU | 7089 | PTC Supply Voltage
9 | 0.5 BN/WH | 585 | Oil Temperature Sensor Signal | 9 | 0.5 BN/WH | 585 | Oil Temperature Sensor Signal
10 | 0.5 OG/BK | 586 | Oil Temperature Low Reference | 10 | 0.5 OG/BK | 586 | Oil Temperature Low Reference
11 | 0.5 OG | 1525 | Steering Wheel Module Shift Solenoid Supply Voltage (1) (M98) | 11 | 0.5 OG | 1525 | Steering Wheel Module Shift Solenoid Supply Voltage (1) (M98)
12 | 0.5 D-BU | 1530 | Transmission Main Pressure Solenoid 5 Volt Reference (M98) | 12 | 0.5 D-BU | 1530 | Transmission Main Pressure Solenoid 5 Volt Reference (M98)
13 | 0.5 D-BU | 6253 | Trasnsmission Input Speed Sensor Ground (M98) | 13 | 0.5 D-BU | 6253 | Trasnsmission Input Speed Sensor Ground (M98)
14 | 0.5 BN/WH | 6254 | Trasnsmission Input Speed Sensor Signal (M98) | 14 | 0.5 BN/WH | 6254 | Trasnsmission Input Speed Sensor Signal (M98)
15 | 0.5 PU/WH | 6282 | Fuel Level Sensor Signal | 15 | 0.5 PU/WH | 6282 | Fuel Level Sensor Signal
16 | 0.5 WH | 1526 | Steering Wheel Module Shift Solenoid Low Reference(M98) | 16 | 0.5 WH | 1526 | Steering Wheel Module Shift Solenoid Low Reference(M98)
17 | 0.5 L-GN | 1527 | Steering Wheel Module Shift Solenoid Supply Voltage (2) (M98) | 17 | 0.5 L-GN | 1527 | Steering Wheel Module Shift Solenoid Supply Voltage (2) (M98)
18 | 0.5 BU | 1528 | Passenger I/P Module Stage 1 Low Reference | 18 | 0.5 BU | 1528 | Passenger I/P Module Stage 1 Low Reference
19 | 0.5 PU | 1529 | Passenger I/P Module Stage 1 5Volt Reference | 19 | 0.5 PU | 1529 | Passenger I/P Module Stage 1 5Volt Reference
20 | 0.35 WH | 5503 | Low Reference | 20 | 0.35 WH | 5503 | Low Reference
21 | 0.5 BN | 323 | Shift Solenoid Supply Voltage (M98) | 21 | 0.5 BN | 323 | Shift Solenoid Supply Voltage (M98)
22 | 0.5 BU/WH | 5502 | Shift Solenoid Supply Voltage 2 (M98) | 22 | 0.5 BU/WH | 5502 | Shift Solenoid Supply Voltage 2 (M98)
23 | 0.5 BN/WH | 379 | Cruise Control Signal | 23 | 0.5 BN/WH | 379 | Cruise Control Signal
24 | 0.5 D-BU | 1319 | Serial Data K-Line | 24 | 0.5 D-BU | 1319 | Serial Data K-Line
25 | 0.5 L-BU | 1937 | Low Reference | 25 | 0.5 L-BU | 1937 | Low Reference
26 | 0.5 BN/WH | 6281 | Fuel Level Sensor Low Reference | 26 | 0.5 BN/WH | 6281 | Fuel Level Sensor Low Reference
27 | 0.5 D-BU | 1936 | Fuel Level Sensor -- Primary | 27 | 0.5 D-BU | 1936 | Fuel Level Sensor -- Primary
28 | 0.5 GY | 324 | Shift Relay Coil Control | 28 | 0.5 GY | 324 | Shift Relay Coil Control
29 | 0.5 YE/BK | 6553 | PTC Supply Voltage | 29 | 0.5 YE/BK | 6553 | PTC Supply Voltage
30 | 0.5 BN/BK | 6357 | Transmission Output Speed Signal Shield | 30 | 0.5 BN/BK | 6357 | Transmission Output Speed Signal Shield
31 | 0.5 PK | 6358 | Transmission Output Speed Signal | 31 | 0.5 PK | 6358 | Transmission Output Speed Signal
32 | 0.5 TN | 2501 | High Speed GM Lan Serial Data - | 32 | 0.5 TN | 2501 | High Speed GM Lan Serial Data -
33 | 0.5 WH/BK | 910 | PTC Request Signal | 33 | 0.5 WH/BK | 910 | PTC Request Signal
34 | 0.5 D-BU | 5985 | Accessory Wakeup Serial Data | 34 | 0.5 D-BU | 5985 | Accessory Wakeup Serial Data
35 | 0.5 TN/BK | 2500 | High Speed GM Lan Serial Data + | 35 | 0.5 TN/BK | 2500 | High Speed GM Lan Serial Data +
36 | 0.5 PK/BK | 5501 | TCC/Clutch Select Solenoid Control | 36 | 0.5 PK/BK | 5501 | TCC/Clutch Select Solenoid Control

#### X102 Forward Lamp Harness to Windshield Washer Harness (Without CE4 or T96 or UFR)

#### Connector Part Information

- OEM: PED 15326849
- Service: N/A
- Description: 12-Way F Sealed

#### Connector Part Information

- OEM: PED 15326854
- Service: N/A
- Description: 12-Way M Sealed

#### X102 Forward Lamp Harness to Windshield Washer Harness (Without CE4 or T96 or UFR)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 PU | 5531 | Hood Closed Signal | 1 | 0.35 PU | 5531 | Hood Closed Signal
2 | 0.35 PU | 1197 | Headlamp Washer Pump Control | 2 | 0.35 PU | 1197 | Headlamp Washer Pump Control
3 | 0.35 D-GN | 392 | Rear Window Washer Pump | 3 | 0.35 D-GN | 392 | Rear Window Washer Pump
0.35 D-GN | 392 | Rear Window Washer Pump
4 | 0.35 BN | 41 | Ignition Voltage | 4 | 0.35 BN | 41 | Ignition Voltage
5 | 0.35 OG/BK | 635-- | Low Reference | 5 | 0.35 OG/BK | 635-- | Low Reference
6 | 0.35 D-GN/WH | 636 | Ambient Air Temp Signal | 6 | 0.35 D-GN/WH | 636 | Ambient Air Temp Signal
7 | 0.3 5BK | 150 | Ground | 7 | 0.3 5BK | 150 | Ground
8 | 0.35 OG | 228 | Windshield Washer Pump Control | 8 | 0.35 OG | 228 | Windshield Washer Pump Control
0.35 OG | 228 | Windshield Washer Pump Control
9 | 0.35 BN/WH | 99 | Windshield Washer Float Level Signal | 9 | 0.35 BN/WH | 99 | Windshield Washer Float level Signal
0.35 BN/WH | 99 | Windshield Washer Float level Signal
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | 0.35 PU/WH | 5203 | Air Quality Sensor Signal | 11 | 0.35 PU/WH | 5203 | Air Quality Sensor Signal
12 | 0.35 BK | 150 | Ground | 12 | 0.35 BK | 150 | Ground

#### X102 Forward Lamp Harness to Windshield Washer Harness (With CE4 or T96 or UFR)

#### Connector Part Information

- OEM: 936777-2
- Service: N/A
- Description: 20-Way F, MTIII/JPT Sealed (BK)

#### Connector Part Information

- OEM: 936780-2
- Service: N/A
- Description: 20-Way M MTIII/JPT Sealed (BK)

#### X102 Forward Lamp Harness to Windshield Washer Harness (With CE4 or T96 or UFR)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 BK | 150 | Ground | 1 | 0.35 BK | 150 | Ground
2 | 0..350OG | 228 | Windshield Washer Fluid Pump Control (CE4) | 2 | 0..350OG | 228 | Windshield Washer Fluid Pump Control (CE4)
3 | 0.35 PU | 5531 | Hood Closed Signal | 3 | 0.35 PU | 5531 | Hood Closed Signal
4 | 0.35 PU/WH | 9382 | 5 Volt Reference | 4 | 0.35 PU/WH | 9382 | 5 Volt Reference
5 | OG/BK | 5214 | Front Parking Sensor Low Reference | 5 | OG/BK | 5214 | Front Parking Sensor Low Reference
6 | 0.35 BK | 150 | Ground | 6 | 0.35 BK | 150 | Ground
7 | 0.35 PU | 34 | Front Fog Lamp Supply Voltage | 7 | 0.35 PU | 34 | Front Fog Lamp Supply Voltage
8 | 0.35 PU | 1197 | Headlamp Washer Pump Control (CE4) | 8 | 0.35 PU | 1197 | Headlamp Washer Pump Control (CE4)
9 | 0.35 GN/WH | 636 | Outside Ambient Air Temperature Sensor Signal | 9 | 0.35 GN/WH | 636 | Outside Ambient Air Temperature Sensor Signal
10 | 0.35 OG/BK | 645 | Sensor Low Reference | 10 | 0.35 OG/BK | 645 | Sensor Low Reference
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | 0.35 BN/WH | 99 | Windshield Washer Fluid Level Sensor Signal (CE4) | 12 | 0.35 BN/WH | 99 | Windshield Washer Fluid Level Sensor Signal (CE4)
13 | 0.35 PU/WH | 5203 | Air Quality Sensor Signal | 13 | 0.35 PU/WH | 5203 | Air Quality Sensor Signal
14 | 0.35 BN/WH | 6547 | Air Quality Sensor Low Reference | 14 | 0.35 BN/WH | 6547 | Air Quality Sensor Low Reference
15 | 0.35 BN | 41 | Ignition Voltage | 15 | 0.35 BN | 41 | Ignition Voltage
16 | 0.35 GN | 392 | Rear Window Washer Pump Control | 16 | 0.35 GN | 392 | Rear Window Washer Pump Control
0.35 GN | 392 | Rear Window Washer Pump Control (CE4)
17 | 0.35 PU/BK | 5218 | Front Parking Right Mid Sensor | 17 | 0.35 PU/BK | 5218 | Front Parking Right Mid Sensor
18 | 0.35 BN/WH | 5217 | Front Parking Right Corner Sensor | 18 | 0.35 BN/WH | 5217 | Front Parking Right Corner Sensor
19 | 0.35 WH | 5216 | Front Parking Left Mid Sensor | 19 | 0.35 WH | 5216 | Front Parking Left Mid Sensor
20 | 0.35 PU/WH | 5215 | Front Parking Left Corner Sensor | 20 | 0.35 PU/WH | 5215 | Front Parking Left Corner Sensor

#### X103 Engine Harness to Fuel Heater Harness (LLW) (RHD)

#### Connector Part Information

- OEM: PED 15401338
- Service: N/A
- Description: 8-Way F 110 Series Sealed (GY)

#### Connector Part Information

- OEM: PED 7282-5684-10
- Service: N/A
- Description: 8-Way M YESC/USCAR ClassIII Series Sealed (GY)

#### X103 Engine Harness to Fuel Heater Harness (LLW) (RHD)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 BK | 250 | Ground | 1 | 0.35 BK | 250 | Ground
2 | 0.35 D-BU | 488 | Fuel Filter Heater Control | 2 | 0.35 D-BU | 488 | Fuel Filter Heater Control
3 | 0.35 GN | 3211 | Fuel Temperature sensor Signal | 3 | 0.35 GN | 3211 | Fuel Temperature sensor Signal
4 | 0.35 BK/WH | 3210 | Low Reference | 4 | 0.35 BK/WH | 3210 | Low Reference
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | 0.35 PK | 539 | Ignition 1 Voltage | 6 | 0.35 PK | 539 | Ignition 1 Voltage
7 | 0.3 WH | 3058 | Water In Fuel Sensor Signal | 7 | 0.3 WH | 3058 | Water In Fuel Sensor Signal
8 | 0.35 BK | 250 | Ground | 8 | 0.35 BK | 250 | Ground

#### X103 Engine Harness to Fuel Heater Harness (LLW) (LHD)

#### Connector Part Information

- OEM: PED 7283-5909-40
- Service: N/A
- Description: 10-Way F 1.5 Series Sealed (L-GY)

#### Connector Part Information

- OEM: PED 7282-5533-40
- Service: N/A
- Description: 10-Way M 1.5 Series Sealed (L-GY)

#### X103 Engine Harness to Fuel Heater Harness (LLW) (LHD)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 WH | 3058 | Water In Fuel Sensor Signal | 1 | 0.35 WH | 3058 | Water In Fuel Sensor Signal
2 | 0.35 BK | 250 | Ground | 2 | 0.35 BK | 250 | Ground
3 | 0.35 PK | 539 | Ignition 1 Voltage | 3 | 0.35 PK | 539 | Ignition 1 Voltage
4 | 0.35 PU | 3044 | Diesel Particulate Filter (DPF) Pressure Sensor 5 V Reference | 4 | 0.35 PU | 3044 | Diesel Particulate Filter (DPF) Pressure Sensor 5 V Reference
5 | 0.35 BK/WH | 3037 | Diesel Particulate Filter (DPF) Pressure Sensor Low Reference | 5 | 0.35 BK/WH | 3037 | Diesel Particulate Filter (DPF) Pressure Sensor Low Reference
6 | 0.35 GN | 3034 | Exhaust Gas Temperature Sensor 1 Signal | 6 | 0.35 GN | 3034 | Exhaust Gas Temperature Sensor 1 Signal
7 | 0.3 5 BK/WH | 3035 | Exhaust Gas Temperature Sensor 1 Low Reference | 7 | 0.3 5 BK/WH | 3035 | Exhaust Gas Temperature Sensor 1 Low Reference
8 | 0.35 GN/BK | 3032 | Exhaust Gas Temperature Sensor 2 Signal | 8 | 0.35 GN/BK | 3032 | Exhaust Gas Temperature Sensor 2 Signal
9 | 0.35 BK | 3033 | Exhaust Gas Temperature Sensor 2 Low Reference | 9 | 0.35 BK | 3033 | Exhaust Gas Temperature Sensor 2 Low Reference
10 | 0.35 GN | 3064 | Diesel Particulate Filter (DPF) Pressure Sensor Signal | 10 | 0.35 GN | 3064 | Diesel Particulate Filter (DPF) Pressure Sensor Signal

#### X104 Engine Harness to Glow Plug Harness (LLW)

#### Connector Part Information

- OEM: 7283-5571-30
- Service: N/A
- Description: 4-Way F YESC/USCAR Class III Series Sealed (BK)

#### Connector Part Information

- OEM: PED 7282-5570-10
- Service: N/A
- Description: 4-Way M YESC Series Sealed (BK)

#### X104 Engine Harness to Glow Plug Harness (LLW)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 GY | 5501 | Glow Plug 4 Battery Voltage | 1 | 0.35 GY | 5501 | Glow Plug 4 Battery Voltage
2 | 0.35 GY | 5501 | Glow Plug 3 Battery Voltage | 2 | 0.35 GY | 5501 | Glow Plug 3 Battery Voltage
3 | 0.35 GY | 5501 | Glow Plug 2 Battery Voltage | 3 | 0.35 GY | 5501 | Glow Plug 2 Battery Voltage
4 | 0.35 GY | 5501 | Glow Plug 1 Battery Voltage | 4 | 0.35 GY | 5501 | Glow Plug 1 Battery Voltage

#### X105 Engine Harness to Exhaust Gas Temperature Harness (LLW) (RHD)

#### Connector Part Information

- OEM: 7283-5571-30
- Service: N/A
- Description: 4-Way F YESC/USCAR Class III Series Sealed (BK)

#### Connector Part Information

- OEM: PED 7282-5570-10
- Service: N/A
- Description: 4-Way M YESC Series Sealed (BK)

#### X105 Engine Harness to Exhaust Gas Temperature Harness (LLW) (RHD)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 GN | 3034 | Exhaust Gas Temperature Sensor 1 Signal | 1 | 0.35 GN | 3034 | Exhaust Gas Temperature Sensor 1 Signal
2 | 0.35 BK/WH | 3035 | Exhaust Gas Temperature Sensor 1 Low Reference | 2 | 0.35 BK/WH | 3035 | Exhaust Gas Temperature Sensor 1 Low Reference
3 | 0.35 GN/BK | 3032 | Exhaust Gas Temperature Sensor 2 Signal | 3 | 0.35 GN/BK | 3032 | Exhaust Gas Temperature Sensor 2 Signal
4 | 0.35 BK | 3033 | Exhaust Gas Temperature Sensor 2 Low Reference | 4 | 0.35 BK | 3033 | Exhaust Gas Temperature Sensor 2 Low Reference

#### X106 Engine Harness to Heated Oxygen Sensor (HO2S) Harness (LU1)

#### Connector Part Information

- OEM: 7283-5571-30
- Service: N/A
- Description: 4-Way F YESC/USCAR Class III Series Sealed (BK)

#### Connector Part Information

- OEM: PED 7282-5570-10
- Service: N/A
- Description: 4-Way M YESC Series Sealed (BK)

#### X106 Engine Harness to Heated Oxygen Sensor (HO2S) Harness (LU1)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2 PU | 6 | Starter Solenoid Crank Voltage | 1 | 2 PU | 6 | Starter Solenoid Crank Voltage
2 | 0.35 PK/BK | 5292 | Ignition 1 Voltage | 2 | 0.35 PK/BK | 5292 | Ignition 1 Voltage
3 | 0.35 BK/WH | 251 | Ground | 3 | 0.35 BK/WH | 251 | Ground
4 | 0.35 PK/BK | 5292 | Ignition 1 Voltage | 4 | 0.35 PK/BK | 5292 | Ignition 1 Voltage
4 | 0.35 YE/GN | 5292 | Ignition 1 Voltage
5 | 0.35 GN | 59 | A/C Compressor Clutch Supply Voltage | 5 | 0.35 GN | 59 | A/C Compressor Clutch Supply Voltage
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | 0.35 PK/BK | 5293 | Ignition 1 Voltage | 7 | 0.35 PK/BK | 5293 | Ignition 1 Voltage
7 | 0.35 RD | 5293 | Ignition 1 Voltage

#### X108 Engine Harness to Fuel Injector Harness (LU1)

#### Connector Part Information

- OEM: PED 1-963214-12
- Service: N/A
- Description: 10-Way F Junior Power Timer Series Sealed (BK)

#### Connector Part Information

- OEM: 1-962352-1
- Service: N/A
- Description: 10-Way M Junior Power Timer Series, Sealed (BK)

#### X108 Engine Harness to Fuel Injector Harness (LU1)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 PK/BK | 5291 | Ignition 1 Voltage | 1 | 0.35 PK/BK | 5291 | Ignition 1 Voltage
2 | 0.35 PK/BK | 5292 | Ignition 1 Voltage | 2 | 0.35 PK/BK | 5292 | Ignition 1 Voltage
3 | 0.35 TN | 1744 | Fuel Injector 1 Control | 3 | 0.35 TN | 1744 | Fuel Injector 1 Control
4 | 0.35 PK/BK | 1746 | Fuel Injector 3 Control | 4 | 0.35 PK/BK | 1746 | Fuel Injector 3 Control
5 | 0.35 TN/WH | 845 | Fuel Injector 5 Control | 5 | 0.35 TN/WH | 845 | Fuel Injector 5 Control
6 | 0.35 L-GN/BK | 1745 | Fuel Injector 2 Control | 6 | 0.35 L-GN/BK | 1745 | Fuel Injector 2 Control
7 | 0.3 5 L-BU/BK | 844 | Fuel Injector 4 Control | 7 | 0.3 5 L-BU/BK | 844 | Fuel Injector 4 Control
8 | 0.35 YE/BK | 846 | Fuel Injector 6 Control | 8 | 0.35 YE/BK | 846 | Fuel Injector 6 Control
9-10 | -- | -- | Not Used | 9-10 | -- | -- | Not Used

#### X201Body Harness to I/P Harness

#### Connector Part Information

- OEM: TYCO 0-1743255-2
- Service: N/A
- Description: 92-Way F Micro-Pack 1.5/2.8 HYB (BK)

#### Connector Part Information

- OEM: TYCO 0-1743251-2
- Service: N/A
- Description: 92-Way M Micro-Pack 1.5/2.8 HYB (BK)

#### X201Body Harness to I/P Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 BN/WH | 771 | Transmission Range Switch Signal A (M98/C105/RHD) | 1 | 0.35 BN/WH | 771 | Transmission Range Switch Signal A (M98/C105/RHD)
1 | 0.35 GY/BK | 2508 | Microphone Signal (UU8/UCY) | 1 | 0.35 GY/BK | 2508 | Microphone Signal (UU8/UCY)
2 | 0.35 L-GN | 200 | Right Front Speaker (+) (1) | 2 | 0.35 L-GN | 200 | Right Front Speaker (+) (1)
3 | 0.35 D-GN | 117 | Right Front Speaker Signal (-) (1) | 3 | 0.35 D-GN | 117 | Right Front Speaker Signal (-) (1)
4 | 0.35 L-BU | 5362 | Incline Sensor Alarm On Signal (AF8) | 4 | 0.35 L-BU | 5362 | Incline Sensor Alarm On Signal (AF8)
5 | 0.35 L-BU | 772 | Transmission Range Switch Signal B (M98/C100/RHD) | 5 | 0.35 L-BU | 772 | Transmission Range Switch Signal B (M98/C100/RHD)
5 | 0.35 BN/BK | 5168 | Power Sounder Enable Signal (C105) | 5 | 0.35 BN/BK | 5168 | Power Sounder Enable Signal (C105)
5 | 0.35 BN/WH | 6433 | CAN Bus High Serial Data (UCY) | 5 | 0.35 BN/WH | 6433 | CAN Bus High Serial Data (UCY)
6 | 0.35 GY | 5248 | Park Assist Alarm Low Reference (UD7) | 6 | 0.35 GY | 5248 | Park Assist Alarm Low Reference (UD7)
6 | 0.35 BN | 5910 | Door Double Lock Actuator Lock Control (C105) | 6 | 0.35 BN | 5910 | Door Double Lock Actuator Lock Control (C105)
7 | 0.35 OG | 1525 | Clutch Pressure Control Solenoid Valve 1 High Control (M98/C105/RHD) | 7 | 0.35 OG | 1525 | Clutch Pressure Control Solenoid Valve 1 High Control (M98/C105/RHD)
7 | 0.35 YE | 5247 | Park Assist Alarm Signal (UD7) | 7 | 0.35 YE | 5247 | Park Assist Alarm Signal (UD7)
8 | 0.35 PU | 1319 | Engine/Radio Serial Data K-Line (UD7) | 8 | 0.35 PU | 1319 | Engine/Radio Serial Data K-Line (UD7)
8 | 0.35 OG | 1525 | Clutch Pressure Control Solenoid Valve 1 High Control (M98/C100/RHD) | 8 | 0.35 OG | 1525 | Clutch Pressure Control Solenoid Valve 1 High Control (M98/C100/RHD)
9 | 0.35Pk | 5068 | Intrusion Sensor Switch Disable Signal (C105/RHD) | 9 | 0.35Pk | 5068 | Intrusion Sensor Switch Disable Signal (C105/RHD)
9 | 0.35 BN/BK | 6724 | Headlamp Washer Pump Switch Signal | 9 | 0.35 BN/BK | 6724 | Headlamp Washer Pump Switch Signal
10 | 0.35 L-BU | 6844 | ABS/TCS Hill Descent Control (F45) | 10 | 0.35 L-BU | 6844 | ABS/TCS Hill Descent Control (F45)
11 | BN/WH | 312 | Right Headlamp Low Beam Supply Voltage (C105/RHD) | 11 | BN/WH | 312 | Right Headlamp Low Beam Supply Voltage (C105/RHD)
11 | 0.35 GY | 773 | Transmission Range Switch Signal C (M98/C100/RHD) | 11 | 0.35 GY | 773 | Transmission Range Switch Signal C (M98/C100/RHD)
11 | 0.35 GY/BK | 7043 | Microphone (+) | 11 | 0.35 GY/BK | 7043 | Microphone (+)
12 | 0.35 WH | 776 | Transmission Range Switch Signal P (M98/C100/RHD) | 12 | 0.35 WH | 776 | Transmission Range Switch Signal P (M98/C100/RHD)
12 | 0.35 WH | 9003 | Drain Wire (C105/RHD) | 12 | 0.35 WH | 9003 | Drain Wire (C105/RHD)
13 | 0.35 BN | 201 | Left Front Speaker (+) (1) | 13 | 0.35 BN | 201 | Left Front Speaker (+) (1)
14 | 0.35 GY | 118 | Left Front Speaker Signal (-) (1) | 14 | 0.35 GY | 118 | Left Front Speaker Signal (-) (1)
15 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage | 15 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage
16 | 0.35 D-BU | 46 | Right Rear Speaker (+) | 16 | 0.35 D-BU | 46 | Right Rear Speaker (+)
17 | 0.35 L-BU | 115 | Right Rear Speaker Signal (-) | 17 | 0.35 L-BU | 115 | Right Rear Speaker Signal (-)
18 | 0.35YE | 116 | Left Rear Speaker Signal (-) | 18 | 0.35YE | 116 | Left Rear Speaker Signal (-)
19 | 0.35 PU/WH | 5203 | Air Quality Sensor Signal | 19 | 0.35 PU/WH | 5203 | Air Quality Sensor Signal
20 | 0.35 GY | 391 | Rear Window Wiper Switch Signal | 20 | 0.35 GY | 391 | Rear Window Wiper Switch Signal
21 | 0.35 D-GN/WH | 636 | Outside Ambient Air Temperature Sensor Signal | 21 | 0.35 D-GN/WH | 636 | Outside Ambient Air Temperature Sensor Signal
22 | 0.35 OG/BK | 645 | Low Reference | 22 | 0.35 OG/BK | 645 | Low Reference
23 | 0.35 WH | 193 | Rear Defog Relay Control | 23 | 0.35 WH | 193 | Rear Defog Relay Control
24 | 0.35 D-GN | 189 | Headlamp Leveling Motor Supply Voltage | 24 | 0.35 D-GN | 189 | Headlamp Leveling Motor Supply Voltage
25 | 0.35 BN/WH | 312 | Right Headlamp Low Beam Supply Voltage (-C105/RHD) | 25 | 0.35 BN/WH | 312 | Right Headlamp Low Beam Supply Voltage (-C105/RHD)
26 | 0.35 GY | 6137 | EVAP Core Temperature Sensor Signal | 26 | 0.35 GY | 6137 | EVAP Core Temperature Sensor Signal
27 | 0.35 OG | 1732 | Electronic Control Unit 12-Volt Reference (3) | 27 | 0.35 OG | 1732 | Electronic Control Unit 12-Volt Reference (3)
28 | 0.35 WH | 639 | Power Sounder (M98/C105/RHD | 28 | 0.35 WH | 639 | Power Sounder (M98/C105/RHD
28 | 0.35 WH | 9003 | Drain Wire (AF8/C100/RHD) | 28 | 0.35 WH | 9003 | Drain Wire (AF8/C100/RHD)
29 | 0.35 YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage | 29 | 0.35 YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage
30 | 0.35 BN/WH | 379 | Cruise Control Clutch Pedal Position Switch Signal (MFN) | 30 | 0.35 BN/WH | 379 | Cruise Control Clutch Pedal Position Switch Signal (MFN)
31 | 0.35 D-BU | 5985 | Accessory Wakup Serial Data (M98/C105/RHD) | 31 | 0.35 D-BU | 5985 | Accessory Wakup Serial Data (M98/C105/RHD)
32 | 0.35 BN | 1149 | Content Theft Horn Control (C105/RHD) | 32 | 0.35 BN | 1149 | Content Theft Horn Control (C105/RHD)
32 | 0.35 YE | 1496 | Mirror Motor Right/Up Control | 32 | 0.35 YE | 1496 | Mirror Motor Right/Up Control
33 | 0.35 BN | 333 | Brake Fluid Level Sensor Signal | 33 | 0.35 BN | 333 | Brake Fluid Level Sensor Signal
34 | 0.35 PU/WH | 5754 | Amplifier Powered Woofer Control (1) (U88) | 34 | 0.35 PU/WH | 5754 | Amplifier Powered Woofer Control (1) (U88)
35 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data (+) (1) | 35 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data (+) (1)
36 | 0.35 PU | 1703 | Variable Effort Steering Speed Sensitive Solenoid Control (NV8) | 36 | 0.35 PU | 1703 | Variable Effort Steering Speed Sensitive Solenoid Control (NV8)
37 | 0.35 YE | 772 | Transmission Range Switch Signal B (M98/C105/RHD) | 37 | 0.35 YE | 772 | Transmission Range Switch Signal B (M98/C105/RHD)
37 | 0.35 PK | 5068 | Intrusion Sensor Switch Disable Signal (AF8/C100/RHD) | 37 | 0.35 PK | 5068 | Intrusion Sensor Switch Disable Signal (AF8/C100/RHD)
38 | 0.5 RD/WH | 2440 | Battery Positive Voltage (M98/C105/RHD) | 38 | 0.5 RD/WH | 2440 | Battery Positive Voltage (M98/C105/RHD)
38 | 0.35 BN/BK | 5168 | Power Sounder Enable Signal (AF8/C100/RHD) | 38 | 0.35 BN/BK | 5168 | Power Sounder Enable Signal (AF8/C100/RHD)
39 | 0.35 L-BU | 659 | Cellular Telephone Voice Low Reference (C105/RHD) | 39 | 0.35 L-BU | 659 | Cellular Telephone Voice Low Reference (C105/RHD)
39 | 0.35 GY | 2373 | Rear Parking Assist Red Indicator Control | 39 | 0.35 GY | 2373 | Rear Parking Assist Red Indicator Control
40 | 0.35 BU | 658 | Cellular Telephone Voice Signal (C105/RHD) | 40 | 0.35 BU | 658 | Cellular Telephone Voice Signal (C105/RHD)
40 | 0.35 PK/BK | 5755 | Amplifier Powered Woofer Control (2) | 40 | 0.35 PK/BK | 5755 | Amplifier Powered Woofer Control (2)
41 | 0.35 BN | 1271 | Accelerator Pedal Position Low Reference (1) | 41 | 0.35 BN | 1271 | Accelerator Pedal Position Low Reference (1)
42 | 0.35 WH/BK | 1164 | Accelerator Pedal Position 5-Volt Reference (1) | 42 | 0.35 WH/BK | 1164 | Accelerator Pedal Position 5-Volt Reference (1)
43 | 0.35 L-BU | 1162 | Accelerator Pedal Position Signal (2) | 43 | 0.35 L-BU | 1162 | Accelerator Pedal Position Signal (2)
44 | 0.35 BN | 1274 | Accelerator Pedal Position 5-Volt Reference (2) | 44 | 0.35 BN | 1274 | Accelerator Pedal Position 5-Volt Reference (2)
45 | 0.35 TN | 2501 | High Speed GMLAN Serial Data (-) (1) | 45 | 0.35 TN | 2501 | High Speed GMLAN Serial Data (-) (1)
46 | 0.35 L-BU | 1738 | Variable Effort Steering Speed Sensitive Solenoid Supply Voltage | 46 | 0.35 L-BU | 1738 | Variable Effort Steering Speed Sensitive Solenoid Supply Voltage
47 | 0.35 GY/BK | 690 | Courtesy Lamp Relay Control (C100/RHD) | 47 | 0.35 GY/BK | 690 | Courtesy Lamp Relay Control (C100/RHD)
47 | 0.35 WH | 776 | Transmission Range Switch Signal P (M98/C105/RHD) | 47 | 0.35 WH | 776 | Transmission Range Switch Signal P (M98/C105/RHD)
48 | 0.35 GY | 773 | Transmission Range Switch Signal C (M98/C105/RHD) | 48 | 0.35 GY | 773 | Transmission Range Switch Signal C (M98/C105/RHD)
48 | 0.35 BN | 5910 | Trailer Fog Lamp | 48 | 0.35 BN | 5910 | Trailer Fog Lamp
49 | 0.35 PU | 1272 | Accelerator Pedal Position Low Reference (2) | 49 | 0.35 PU | 1272 | Accelerator Pedal Position Low Reference (2)
50 | 0.35 D-BU | 1161 | Accelerator Pedal Position Signal (1) | 50 | 0.35 D-BU | 1161 | Accelerator Pedal Position Signal (1)
51 | 0.35 BN | 199 | Left Rear Speaker (+) | 51 | 0.35 BN | 199 | Left Rear Speaker (+)
52 | 0.35 BN/WH | 99 | Windshield Washer Fluid Level Sensor Signal | 52 | 0.35 BN/WH | 99 | Windshield Washer Fluid Level Sensor Signal
53 | 0.35 WH | 81 | Left Mirror Motor Right Control (C100/RHD) | 53 | 0.35 WH | 81 | Left Mirror Motor Right Control (C100/RHD)
53 | 0.35 BN | 1391 | Driver Door Unlock Relay Control (C105/RHD) | 53 | 0.35 BN | 1391 | Driver Door Unlock Relay Control (C105/RHD)
54 | 0.35 L-GN | 89 | Left Mirror Motor Down Control | 54 | 0.35 L-GN | 89 | Left Mirror Motor Down Control
54 | 0.35 GN/WH | 5842 | Auxiliary Audio Screen (2) (C105/RHD) | 54 | 0.35 GN/WH | 5842 | Auxiliary Audio Screen (2) (C105/RHD)
55 | 0.35 BU | 6253 | Low Reference (M98/C100/RHD) | 55 | 0.35 BU | 6253 | Low Reference (M98/C100/RHD)
56 | 0.35 TN | 2501 | High Speed GMLAN Serial Data (-) (1) | 56 | 0.35 TN | 2501 | High Speed GMLAN Serial Data (-) (1)
57 | WH/BK | 910 | PTC Heater Request Signal | 57 | WH/BK | 910 | PTC Heater Request Signal
57 | 0.35 WH | 1310 | EVAP Cannister Vent Solenoid Control (NQU) | 57 | 0.35 WH | 1310 | EVAP Cannister Vent Solenoid Control (NQU)
58 | 0.5 RD/WH | 540 | Battery Positive Voltage | 58 | 0.5 RD/WH | 540 | Battery Positive Voltage
59 | 0.35 OG/WH | 881 | Right Mirror Motor Right Control (C100/RHD) | 59 | 0.35 OG/WH | 881 | Right Mirror Motor Right Control (C100/RHD)
59 | 0.35 BN/WH | 5169 | Mid Speed GMLAN Serial Data Bus+ (C105/RHD) | 59 | 0.35 BN/WH | 5169 | Mid Speed GMLAN Serial Data Bus+ (C105/RHD)
60 | 0.35 PU/WH | 889 | Right Mirror Motor Down Control (C100/RHD) | 60 | 0.35 PU/WH | 889 | Right Mirror Motor Down Control (C100/RHD)
60 | 0.35 BN | 5170 | Mid Speed GMLAN Serial Data Bus- (C105/RHD) | 60 | 0.35 BN | 5170 | Mid Speed GMLAN Serial Data Bus- (C105/RHD)
61 | 0.35 GY | 324 | Shift Relay Coil Supply Voltage (C100/RHD) | 61 | 0.35 GY | 324 | Shift Relay Coil Supply Voltage (C100/RHD)
61 | 0.35L-GN | 5839 | Left Auxiliary Audio Signal (2) (C105/RHD) | 61 | 0.35L-GN | 5839 | Left Auxiliary Audio Signal (2) (C105/RHD)
62 | 0.35 PU | 328 | Interior Lamp Defeat Switch Signal | 62 | 0.35 PU | 328 | Interior Lamp Defeat Switch Signal
63 | 0.35 BN | 4 | Accessory Voltage | 63 | 0.35 BN | 4 | Accessory Voltage
64 | 0.35 D-BU | 6189 | Lift Glass/Trunk Interior Release Signal | 64 | 0.35 D-BU | 6189 | Lift Glass/Trunk Interior Release Signal
65 | 0.35 WH | 5190 | Trailer Fog Lamp (C105) | 65 | 0.35 WH | 5190 | Trailer Fog Lamp (C105)
65 | 0.35 BN/WH | 6254 | Input Speed Sensor Signal (M98/C100/RHD) | 65 | 0.35 BN/WH | 6254 | Input Speed Sensor Signal (M98/C100/RHD)
66 | 0.35 D-BU | 5992 | Trailer Connected Signal (C105) | 66 | 0.35 D-BU | 5992 | Trailer Connected Signal (C105)
67 | 0.35 BN/WH | 585 | Transmission Fluid Temperature Sensor Signal (C100/RHD) | 67 | 0.35 BN/WH | 585 | Transmission Fluid Temperature Sensor Signal (C100/RHD)
67 | 0.35 BN | 28 | Horn Relay Control (C105) | 67 | 0.35 BN | 28 | Horn Relay Control (C105)
67 | 0.35 YE | 1860 | Front Center Speaker (+) (UV8/UCY) | 67 | 0.35 YE | 1860 | Front Center Speaker (+) (UV8/UCY)
68 | 0.35 BN | 28 | Horn Relay Control (C100) | 68 | 0.35 BN | 28 | Horn Relay Control (C100)
68 | 0.35 GN/WH | 5841 | Right Auxiliary Audio Signal (2) (C105) | 68 | 0.35 GN/WH | 5841 | Right Auxiliary Audio Signal (2) (C105)
69 | 0.35 GN/WH | 762 | A/C Request Signal | 69 | 0.35 GN/WH | 762 | A/C Request Signal
70 | 0.35 PK/BK | 5501 | TCC Enable Solenoid Valve High Control (M98/C100/RHD) | 70 | 0.35 PK/BK | 5501 | TCC Enable Solenoid Valve High Control (M98/C100/RHD)
70 | 0.35 YE | 5842 | Auxiliary Audio Screen (2) (C105/LHD) | 70 | 0.35 YE | 5842 | Auxiliary Audio Screen (2) (C105/LHD)
71 | 0.35 BU/WH | 5502 | TCC Enable Solenoid Valve Low Control (M98/C100/RHD) | 71 | 0.35 BU/WH | 5502 | TCC Enable Solenoid Valve Low Control (M98/C100/RHD)
72 | 0.35 BU | 1530 | Transmission Mainline Pressure Solenoid Control (M98/C100/RHD) | 72 | 0.35 BU | 1530 | Transmission Mainline Pressure Solenoid Control (M98/C100/RHD)
72 | 0.35 BN/WH | 6547 | Battery Module Temperature Signal (11) (C105) | 72 | 0.35 BN/WH | 6547 | Battery Module Temperature Signal (11) (C105)
73 | 0.35 L-BU | 5986 | Serial Data Communication Enable | 73 | 0.35 L-BU | 5986 | Serial Data Communication Enable
74 | 0.35 GN/WH | 817 | Vehicle Speed Signal (C105) | 74 | 0.35 GN/WH | 817 | Vehicle Speed Signal (C105)
74 | 0.35 WH | 5503 | Transmission Mainline Pressure Solenoid Low Reference (M98/C100/RHD) | 74 | 0.35 WH | 5503 | Transmission Mainline Pressure Solenoid Low Reference (M98/C100/RHD)
75 | 0.35 BN | 323 | Shift Solenoid Supply Voltage (C100/RHD) | 75 | 0.35 BN | 323 | Shift Solenoid Supply Voltage (C100/RHD)
75 | 0.35 YE/BK | 693 | Cellular Telephone Mute Signal (C105) | 75 | 0.35 YE/BK | 693 | Cellular Telephone Mute Signal (C105)
76 | 0.35 PK | 1963 | Folding Mirror Extend Motor Relay Control | 76 | 0.35 PK | 1963 | Folding Mirror Extend Motor Relay Control
77 | 0.35 BN | 683 | Rear Defog Indicator Supply Voltage | 77 | 0.35 BN | 683 | Rear Defog Indicator Supply Voltage
78 | 0.35 GN/BK | 690 | Courtesy Lamp Supply Voltage (C105) | 78 | 0.35 GN/BK | 690 | Courtesy Lamp Supply Voltage (C105)
79 | 0.35 L-GN | 24 | Backup Lamp Supply Voltage (UCY) | 79 | 0.35 L-GN | 24 | Backup Lamp Supply Voltage (UCY)
79 | 0.35 BN/BK | 6357 | Output Speed Shielded Signal (C100/RHD) | 79 | 0.35 BN/BK | 6357 | Output Speed Shielded Signal (C100/RHD)
79 | 0.35 WH | 9004 | Shield Wire (C105) | 79 | 0.35 WH | 9004 | Shield Wire (C105)
80 | 0.35 PK | 3022 | Steering Wheel Module Stage 2 Low Control (F45) | 80 | 0.35 PK | 3022 | Steering Wheel Module Stage 2 Low Control (F45)
81 | 0.35 WH | 3023 | Steering Wheel Module State 2 High Control (F45) | 81 | 0.35 WH | 3023 | Steering Wheel Module State 2 High Control (F45)
82 | 0.35 L-BU | 187 | Rear Fog Lamp Switch Signal | 82 | 0.35 L-BU | 187 | Rear Fog Lamp Switch Signal
83 | 0.35 L-BU | 2088 | Combined Vehicle Inertial Sensor Low Reference | 83 | 0.35 L-BU | 2088 | Combined Vehicle Inertial Sensor Low Reference
84 | 0.35 D-GN | 2087 | Combined Vehicle Inertial Sensor Supply Voltage | 84 | 0.35 D-GN | 2087 | Combined Vehicle Inertial Sensor Supply Voltage
85 | 0.35 BN/WH | 771 | Transmission Range Switch Signal A (M98/C100/RHD) | 85 | 0.35 BN/WH | 771 | Transmission Range Switch Signal A (M98/C100/RHD)
85 | 0.35 BN | 5852 | Rear Park Assist LED Disable Signal (C105) | 85 | 0.35 BN | 5852 | Rear Park Assist LED Disable Signal (C105)
86 | 0.35 OG/BK | 586 | Transmission Fluid Temperature Sensor Low Reference (M98/C100/RHD) | 86 | 0.35 OG/BK | 586 | Transmission Fluid Temperature Sensor Low Reference (M98/C100/RHD)
86 | 0.35 L-BU | 1960 | Front Center Speaker (-) (UV8/UCY) | 86 | 0.35 L-BU | 1960 | Front Center Speaker (-) (UV8/UCY)
86 | 0.35 GN | 2555 | Rear Park Assist Disable Signal (C105) | 86 | 0.35 GN | 2555 | Rear Park Assist Disable Signal (C105)
87 | 0.35 D-GN/WH | 817 | Vehicle Speed Signal | 87 | 0.35 D-GN/WH | 817 | Vehicle Speed Signal
88 | 0.35 BN/WH | 753 | Steering Wheel Module High Signal | 88 | 0.35 BN/WH | 753 | Steering Wheel Module High Signal
89 | 0.35 OG/BK | 752 | Steering Wheel Module Low Signal | 89 | 0.35 OG/BK | 752 | Steering Wheel Module Low Signal
90 | 0.35 D-BU | 903 | Park Assist Alarm Volt Reference (C100/UD7) | 90 | 0.35 D-BU | 903 | Park Assist Alarm Volt Reference (C100/UD7)
91 | 0.35 L-BU | 1134 | Park Brake Switch Signal (UCY) | 91 | 0.35 L-BU | 1134 | Park Brake Switch Signal (UCY)
91 | 0.35 PK | 6358 | Output Speed Signal (C100/RHD) | 91 | 0.35 PK | 6358 | Output Speed Signal (C100/RHD)
92 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data (+) | 92 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data (+)

#### X202 I/P Harness to Body Harness (C100)

#### Connector Part Information

- OEM: TYCO 936196-1
- Service: N/A
- Description: 12-Way F Unsealed

#### Connector Part Information

- OEM: TYCO 936207-1
- Service: N/A
- Description: 12-Way M Unsealed

#### X202 I/P Harness to Body Harness (C100)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 D-BU | 658 | Cellular Telephone Voice Signal (UV8/C100/LHD) | 1 | 0.35 D-BU | 658 | Cellular Telephone Voice Signal (UV8/C100/LHD)
1 | 0.35 RD/WH | 2440 | Battery Positive Voltage (RHD) | 1 | 0.35 RD/WH | 2440 | Battery Positive Voltage (RHD)
2 | 0.35 PK | 639 | Run/Crank Ignition 1 Voltage (RHD) | 2 | 0.35 PK | 639 | Run/Crank Ignition 1 Voltage (RHD)
3 | 0.35 D-GN | 654 | Cellular Telephone Microphone Low Reference (UV8) | 3 | 0.35 D-GN | 654 | Cellular Telephone Microphone Low Reference (UV8)
4 | 0.35 GY | 655 | Cellular Telephone Microphone Signal (UV8) | 4 | 0.35 GY | 655 | Cellular Telephone Microphone Signal (UV8)
4 | 0.35 D-BU | 5985 | Accessory Wakeup Serial Data (RHD) | 4 | 0.35 D-BU | 5985 | Accessory Wakeup Serial Data (RHD)
5 | 0.35 PK | 1155 | Audio Handset Low Reference (UV8) | 5 | 0.35 PK | 1155 | Audio Handset Low Reference (UV8)
6 | 0.35 L-BU | 659 | Cellular Telephone Voice Low Reference (UV8) | 6 | 0.35 L-BU | 659 | Cellular Telephone Voice Low Reference (UV8)
6 | 0.35 PU | 1529 | Shift Solenoid Supply Voltage (5) (RHD) | 6 | 0.35 PU | 1529 | Shift Solenoid Supply Voltage (5) (RHD)
7 | 0.35 D-BU | 1528 | Shift Solenoid Supply Voltage (4) (RHD) | 7 | 0.35 D-BU | 1528 | Shift Solenoid Supply Voltage (4) (RHD)
7 | 0.35 D-GN | 1795 | Right Subwoofer Speaker (+) (U88) | 7 | 0.35 D-GN | 1795 | Right Subwoofer Speaker (+) (U88)
8 | 0.35 L-GN | 1527 | Shift Solenoid Supply Voltage (3) (RHD) | 8 | 0.35 L-GN | 1527 | Shift Solenoid Supply Voltage (3) (RHD)
9 | 0.35 L-BU | 315 | Right Subwoofer Speaker (-) (U88) | 9 | 0.35 L-BU | 315 | Right Subwoofer Speaker (-) (U88)
9 | 0.35 WH | 1526 | Shift Solenoid Supply Voltage (2) (RHD) | 9 | 0.35 WH | 1526 | Shift Solenoid Supply Voltage (2) (RHD)
10 | 0.35 D-BU | 1154 | Audio Handset Earpiece Signal (UV8) | 10 | 0.35 D-BU | 1154 | Audio Handset Earpiece Signal (UV8)
11 | 0.35 GY/BK | 2520 | Transceiver Low Reference (UV8) | 11 | 0.35 GY/BK | 2520 | Transceiver Low Reference (UV8)
12 | 0.35 PK | 1155 | Audio Handset Low Reference (UV8) | 12 | 0.35 PK | 1155 | Audio Handset Low Reference (UV8)

#### X202 I/P Harness to Body Harness (C105/RHD/M98)

#### Connector Part Information

- OEM: TYCO 936201-1
- Service: N/A
- Description: 16-Way F 090III Series (NA)

#### Connector Part Information

- OEM: TYCO 936211-1
- Service: N/A
- Description: 16-Way M 090III Series (NA)

#### X202 I/P Harness to Body Harness (C105/RHD/M98)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 BN/BK | 6357 | Output Speed Shielded Signal | 1 | 0.35 BN/BK | 6357 | Output Speed Shielded Signal
2 | 0.35 D-BU | 6253 | Transmission Input Speed Sensor Ground | 2 | 0.35 D-BU | 6253 | Transmission Input Speed Sensor Ground
3 | 0.35 BN/WH | 585 | Transmission Oil Temperature Sensor Signal | 3 | 0.35 BN/WH | 585 | Transmission Oil Temperature Sensor Signal
4 | 0.35 OG/BK | 586 | Transmission Oil Temperature Sensor Low Reference | 4 | 0.35 OG/BK | 586 | Transmission Oil Temperature Sensor Low Reference
5 | 0.35 WH | 1526 | Shift Solenoid Supply Voltage (2) | 5 | 0.35 WH | 1526 | Shift Solenoid Supply Voltage (2)
6 | 0.35 D-BU | 1528 | Shift Solenoid Supply Voltage (4) | 6 | 0.35 D-BU | 1528 | Shift Solenoid Supply Voltage (4)
7 | 0.35 PK/BK | 5501 | TCC/Clutch Select Solenoid Control | 7 | 0.35 PK/BK | 5501 | TCC/Clutch Select Solenoid Control
8 | 0.35 WH | 5503 | Transmission Mainline Pressure Solenoid Low Reference | 8 | 0.35 WH | 5503 | Transmission Mainline Pressure Solenoid Low Reference
9 | 0.35 PK | 6358 | Output Speed Signal | 9 | 0.35 PK | 6358 | Output Speed Signal
10 | 0.35 BN/WH | 6254 | Transmission Input Speed Sensor Signal | 10 | 0.35 BN/WH | 6254 | Transmission Input Speed Sensor Signal
11 | 0.35 BN | 323 | Shift Solenoid Supply Voltage | 11 | 0.35 BN | 323 | Shift Solenoid Supply Voltage
12 | 0.35 GN | 324 | Shift Relay Coil Control | 12 | 0.35 GN | 324 | Shift Relay Coil Control
13 | 0.35 L-GN | 1527 | Shift Solenoid Supply Voltage (3) | 13 | 0.35 L-GN | 1527 | Shift Solenoid Supply Voltage (3)
14 | 0.35 YE | 1529 | Shift Solenoid Supply Voltage (5) | 14 | 0.35 YE | 1529 | Shift Solenoid Supply Voltage (5)
15 | 0.35 BU/WH | 5502 | TCC/Clutch Select Solenoid Low Reference | 15 | 0.35 BU/WH | 5502 | TCC/Clutch Select Solenoid Low Reference
16 | 0.35 BU | 1530 | Transmission Mainline Pressure Solenoid Control | 16 | 0.35 BU | 1530 | Transmission Mainline Pressure Solenoid Control

#### X203 Inflatable Restraint Harness to I/P Harness

#### Connector Part Information

- OEM: TYCO 936240-1
- Service: N/A
- Description: 6-Way F 090III Unsealed

#### Connector Part Information

- OEM: TYCO 936230-1
- Service: N/A
- Description: 6-Way M 090III Unsealed

#### X203 Inflatable Restraint Harness to I/P Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data | 3 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
4 | 0.35 PK | 439 | Ignition 1 Voltage | 4 | 0.35 PK | 439 | Ignition 1 Voltage
5 | 0.35 BN/WH | 351 | Ground | 5 | 0.35 BN/WH | 351 | Ground
6 | 0.35 RD/WH | 740 | Battery Positive Voltage | 6 | 0.35 RD/WH | 740 | Battery Positive Voltage

#### X301 Body Harness to Console Harness (C100)

#### Connector Part Information

- OEM: TYCO 936196-1
- Service: N/A
- Description: 12-Way F 090III Unsealed

#### Connector Part Information

- OEM: TYCO 936207-1
- Service: N/A
- Description: 12-Way M 090III Unsealed

#### X301 Body Harness to Console Harness (C100)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 D-BU | 1154 | Audio Handset Earpiece Signal | 1 | 0.35 D-BU | 1154 | Audio Handset Earpiece Signal
2 | 0.35 BK | 450 | Ground | 2 | 0.35 BK | 450 | Ground
3 | 0.35 RD/WH | 2740 | Battery Positive Voltage | 3 | 0.35 RD/WH | 2740 | Battery Positive Voltage
4 | 0.35 PK | 1550 | Audio Handset Low Reference | 4 | 0.35 PK | 1550 | Audio Handset Low Reference
5 | 0.35 D-GN | 654 | Cellular Phone Microphone Low | 5 | 0.35 D-GN | 654 | Cell Phone MIC Low Reference
6 | 0.35 GY/BK | 2520 | Transceiver Low Reference | 6 | 0.35 GY/BK | 2520 | Transceiver Low Reference
7 | 0.35 PK | 1155 | Audio Handset Low Reference | 7 | 0.35 PK | 1155 | Audio Handset Low Reference
8 | 0.35 L-BU | 1505 | Passenger Heated Seat Switch Signal | 8 | 0.35 L-BU | 1505 | Passenger Heated Seat Switch Signal
9 | 0.35 L-BU | 1462 | Heated Seat Switch Signal | 9 | 0.35 L-BU | 1462 | Heated Seat Switch Signal
10 | 0.35 YE | 1491 | Backlight Lamp Control | 10 | 0.35 YE | 1491 | Backuplight Lamp Control
11 | 0.35 BN | 241 | Run Ignition 3 Voltage | 11 | 0.35 BN | 241 | Run Ignition 3 Voltage
12 | 0.35 GY | 655 | Cellular Phone Microphone Signal | 12 | 0.35 GY | 655 | Cell Phone Microphone Low Reference

#### X301 Body Harness to Console Harness (UWA)(C105)

#### Connector Part Information

- OEM: TYCO 936199-1
- Service: N/A
- Description: 14-Way F 090 series (NA)

#### Connector Part Information

- OEM: TYCO 936207-1
- Service: N/A
- Description: 14-Way M 090 series (NA)

#### X301 Body Harness to Console Harness (UWA)(C105)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 GY | 7156 | Comm Box RX + Serial Data | 1 | 0.35 GY | 7156 | Comm Box RX + Serial Data
2 | 0.35 BK | 7155 | Comm Box TX + Serial Data | 2 | 0.35 BK | 7155 | Comm Box TX + Serial Data
3 | 0.35 RD | 7150 | Switch Signal | 3 | 0.35 RD | 7150 | Switch Signal
4 | 0.35 PU | 7148 | Mobile Phone SNDREQ Signal | 4 | 0.35 PU | 7148 | Mobile Phone SNDREQ Signal
5 | 0.35 BN | 7144 | Mobile Phone Audio Output Minus Signal | 5 | 0.35 BN | 7144 | Mobile Phone Audio Output Minus Signal
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | 0.35 PK | 7152 | Comm Box RX Serial Data | 7 | 0.35 PK | 7152 | Comm Box RX Serial Data
8 | 0.35 PU | 7309 | Communication Box TX Serial Data | 8 | 0.35 PU | 7309 | Communication Box TX Serial Data
9 | 0.35 BK | 51 | Ground | 9 | 0.35 BK | 51 | Ground
10 | 0.35 GN | 7149 | Communication Box Mic Output Minus Signal | 10 | 0.35 GN | 7149 | Communication Box Mic Output Minus Signal
11 | 0.35 YE | 7154 | Comm Box Mic OT Plus Signal | 11 | 0.35 YE | 7154 | Comm Box Mic OT Plus Signal
12 | 0.35 OG | 7153 | Mobile Phone Current Limited Supply Voltage | 12 | 0.35 OG | 7153 | Mobile Phone Current Limited Supply Voltage
13 | 0.35 WH | 7147 | Mobile Phone Audio Output Plus Signal | 13 | 0.35 WH | 7147 | Mobile Phone Audio Output Plus Signal
14 | -- | -- | Not Used | 14 | -- | -- | Not Used

#### X302 Body Harness to Inflatable Restraint Roof Rail Module Harness - Left

#### Connector Part Information

- OEM: FCI 6020-1704
- Service: N/A
- Description: 2-Way F SICMAIII Unsealed

#### Connector Part Information

- OEM: FCI 6030-1104
- Service: N/A
- Description: 2-Way M SICMAIII Unsealed

#### X302 Body Harness to Inflatable Restraint Roof Rail Module Harness - Left

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 PK | 5020 | LF Roof Rail Module High | 1 | 0.35 PK | 5020 | LF Roof Rail Module High
2 | 0.35 PU/WH | 5019 | LF Roof Rail Module Low | 2 | 0.35 PU/WH | 5019 | LF Roof Rail Module Low

#### X303 Body Harness to Inflatable Restraint Roof Rail Module Harness - Right

#### Connector Part Information

- OEM: FCI 6020-1704
- Service: N/A
- Description: 2-Way F SICMAIII Unsealed

#### Connector Part Information

- OEM: FCI 6030-1104
- Service: N/A
- Description: 2-Way M SICMAIII Unsealed

#### X303 Body Harness to Inflatable Restraint Roof Rail Module Harness - Right

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 YE/BK | 5021 | RF Roof Rail Module High | 1 | 0.35 YE/BK | 5021 | RF Roof Rail Module High
2 | 0.35 WH/BK | 5022 | RF Roof Rail Module Low | 2 | 0.35 WH/BK | 5022 | RF Roof Rail Module Low

#### X306 Body Harness to Console Harness (C105)

#### Connector Part Information

- OEM: TYCO 936199-1
- Service: N/A
- Description: 16-Way F 090 series (NA)

#### Connector Part Information

- OEM: TYCO 936207-1
- Service: N/A
- Description: 16-Way M 090 series (NA)

#### X306 Body Harness to Console Harness (C105)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 BU/WH | 1382 | LED Dimming Signal | 1 | 0.35 BU/WH | 1382 | LED Dimming Signal
2 | 0.35 BK | 550 | Ground | 2 | 0.35 BK | 550 | Ground
3 | 0.35 RD/WH | 2740 | Battery Positive Voltage | 3 | 0.35 RD/WH | 2740 | Battery Positive Voltage
4 | 0.35 RD/WH | 2640 | Battery Positive Voltage | 4 | 0.35 RD/WH | 2640 | Battery Positive Voltage
5 | 0.35 PU | 6172 | Driver Heated Seat Switch Back Cushion Signal | 5 | 0.35 PU | 6172 | Driver Heated Seat Switch Back Cushion Signal
6 | 0.35 GN | 1661 | Driver Heated Seat High Indicator Control | 6 | 0.35 GN | 1661 | Driver Heated Seat High Indicator Control
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control | 8 | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control
9 | 0.35 L-BU | 1662 | Driver Heated Seat Low Indicator Control | 9 | 0.35 L-BU | 1662 | Driver Heated Seat Low Indicator Control
10 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal | 10 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal
11 | 0.35 YE | 1491 | Backlight Lamp Control | 11 | 0.35 YE | 1491 | Backlight Lamp Control
12 | 0.35 BN | 41 | Run Ignition 3 Voltage | 12 | 0.35 BN | 41 | Run Ignition 3 Voltage
13 | 0.35 YE | 1685 | Passenger Heated Seat High Indicator Control | 13 | 0.35 YE | 1685 | Passenger Heated Seat High Indicator Control
14 | WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control | 14 | WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control
15 | 0.35 BN | 1686 | Passenger Heated Seat Low Indicator Control | 15 | 0.35 BN | 1686 | Passenger Heated Seat Low Indicator Control
16 | -- | -- | Not Used | 16 | -- | -- | Not Used

#### X402 Body Harness to Lift Gate Harness

#### Connector Part Information

- OEM: MOLEX 35896-2010
- Service: N/A
- Description: 20-Way F 090II Unsealed

#### Connector Part Information

- OEM: MOLEX 35897-2010
- Service: N/A
- Description: 20-Way M 090II Unsealed

#### X402 Body Harness to Lift Gate Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | 0.35 BK | 650 | Ground | 2 | 0.35 BK | 650 | Ground
3 | 0.35 D-GN | 392 | Rear Window Washer Pump Control | 3 | 0.35 D-GN | 392 | Rear Window Washer Pump Control
4 | 0.35 RD/WH | 2240 | Battery Positive Voltage | 4 | 0.35 RD/WH | 2240 | Battery Positive Voltage
5 | 0.35 PU | 293 | Rear Defog Elemement Supply Voltage | 5 | 0.35 PU | 293 | Rear Defog Elemement Supply Voltage
6 | 0.35 PU | 709 | Left Park Lamp Supply Voltage | 6 | 0.35 PU | 709 | Left Park Lamp Supply Voltage
7 | 0.35 OG | 6201 | Camera Supply Voltage (UVC) | 7 | 0.35 OG | 6201 | Camera Supply Voltage (UVC)
8 | 0.35 BN | 6188 | Lift Glass/Trunk MTR Release Control | 8 | 0.35 BN | 6188 | Lift Glass/Trunk MTR Release Control
9 | 0.35 GY | 391 | Rear Window Wiper Switch Signal | 9 | 0.35 GY | 391 | Rear Window Wiper Switch Signal
10 | 0.35 BN/BK | 6202 | Camera Ground (UVC) | 10 | 0.35 BN/BK | 6202 | Camera Ground (UVC)
11 | 0.35 GY | 6208 | Coaxial Camera Signal (UVC) | 11 | 0.35 GY | 6208 | Coaxial Camera Signal (UVC)
12 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage | 12 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | 0.35 PK/BK | 1303 | Liftgate Ajar Switch Signal (1) | 14 | 0.35 PK/BK | 1303 | Liftgate Ajar Switch Signal (1)
15 | 0.35 BN | 294 | Door Lock Actuator Unlock Control | 15 | 0.35 BN | 294 | Door Lock Actuator Unlock Control
16 | 0.35 GY | 295 | Door Lock Actuator Lock Control | 16 | 0.35 GY | 295 | Door Lock Actuator Lock Control
17 | 0.35 WH | 6798 | Camera Video Signal (UVC) | 17 | 0.35 WH | 6798 | Camera Video Signal (UVC)
18 | 0.35 YE | 6799 | Camera Shield (UVC) | 18 | 0.35 YE | 6799 | Camera Shield (UVC)
19 | 0.35 OG | 9000 | Rear Wiper Auto On Signal | 19 | 0.35 OG | 9000 | Rear Wiper Auto On Signal
20 | 0.35 BN | 305 | Trunk Key Switch Signal | 20 | 0.35 BN | 305 | Trunk Key Switch Signal

#### X405 Body Harness to Rear Object Sensor Harness

#### Connector Part Information

- OEM: AMP 368530-1
- Service: N/A
- Description: 6-Way F Sealed

#### Connector Part Information

- OEM: AMP 174264-2
- Service: N/A
- Description: 6-Way M Sealed

#### X405 Body Harness to Rear Object Sensor Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | OG | 2376 | LH Object Signal | 1 | OG | 2376 | LH Object Signal
2 | GY | 2379 | Low Reference | 2 | GY | 2379 | Low Reference
3 | YE | 2375 | L-Center Object Signal | 3 | YE | 2375 | L-Center Object Signal
4 | PU | 2378 | R Center Object Signal | 4 | PU | 2378 | R Center Object Signal
5 | GY/BK | 2379 | Low Reference | 5 | GY/BK | 2379 | Low Reference
6 | D-GN | 2377 | RH Object Signal | 6 | D-GN | 2377 | RH Object Signal

### X436 - Object Alarm Module Patch Harness Ground (with GFP)

#### Connector Part Information

- OEM:
- Service: See Catalog
- Description: 1-Way F (WH)

#### Connector Part Information

- OEM:
- Service: See Catalog
- Description: 1-Way M (WH)

#### X436 - Object Alarm Module Patch Harness Ground (with GFP)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 8 | Ground | 1 | BK | 2 | Ground

### X437 - Object Alarm Module Patch Harness (with GFP)

#### Connector Part Information

- OEM:
- Service: See Catalog
- Description: 2-Way F (WH)

#### Connector Part Information

- OEM:
- Service: See Catalog
- Description: 2-Way M (WH)

#### X437 - Object Alarm Module Patch Harness (with GFP)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 8 | Ground | 1 | BK | 8 | Ground
2 | RD | 3 | 12-Volt Signal | 2 | RD | 3 | 12-Volt Signal

#### X901 Lift Gate Harness to Lift GateJumper Harness

#### Connector Part Information

- OEM: TYCO 936199-1
- Service: N/A
- Description: 14-Way F 090III Unsealed

#### Connector Part Information

- OEM: TYCO 936209-1
- Service: N/A
- Description: 14-Way M 090III Unsealed

#### X901 Lift Gate Harness to Lift Gate Jumper Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 RD/WH | 2240 | Battery Positive Voltage | 1 | 0.35 RD/WH | 2240 | Battery Positive Voltage
2 | 0.35 PK/BK | 1303 | Liftgate Ajar Switch Signal (1) | 2 | 0.35 PK/BK | 1303 | Liftgate Ajar Switch Signal (1)
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | 0.35 PU | 709 | Left Park Lamp Supply Voltage | 4 | 0.35 PU | 709 | Left Park Lamp Supply Voltage
5 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage | 5 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage
6 | 0.35 D-GN | 392 | Rear Window Washer Pump Control | 6 | 0.35 D-GN | 392 | Rear Window Washer Pump Control
7 | 0.35 GY | 391 | Rear Window Wiper Switch Signal | 7 | 0.35 GY | 391 | Rear Window Wiper Switch Signal
8 | 0.35 OG | 9000 | Rear Wiper Auto On Signal | 8 | 0.35 OG | 9000 | Rear Wiper Auto On Signal
9 | 0.35 BN | 305 | Trunk Key Switch Signal | 9 | 0.35 BN | 305 | Trunk Key Switch Signal
10 | 0.35 BN | 6188 | Lift Glass/Trunk MTR Release | 10 | 0.35 BN | 6188 | Lift Glass/Trunk MTR Release
11 | 0.35 BK | 650 | Ground | 11 | 0.35 BK | 650 | Ground
12 | 0.35 GY | 295 | Door Lock Actuator Lock Control | 12 | 0.35 GY | 295 | Door Lock Actuator Lock Control
13 | 0.35 BN | 294 | Door Lock Actuator Unlock Control | 13 | 0.35 BN | 294 | Door Lock Actuator Unlock Control
14 | 0.35 PU | 293 | Rear Defog Element Supply Voltage | 14 | 0.35 PU | 293 | Rear Defog Element Supply Voltage

#### X902 Lift Gate Harness to Rear View Camera Harness

#### Connector Part Information

- OEM: AMP 936230-1
- Service: N/A
- Description: 6-Way F Unsealed

#### Connector Part Information

- OEM: AMP 936240-1
- Service: N/A
- Description: 6-Way M Unsealed

#### X902 Lift Gate Harness to Rear View Camera Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | OG | 6201 | Camera Supply Voltage | 1 | OG | 6201 | Camera Supply Voltage
2 | BN/BK | 6202 | Camera Ground | 2 | BN/BK | 6202 | Camera Ground
3 | GR | 6208 | Coaxial Camera Signal | 3 | GR | 6208 | Coaxial Camera Signal
4 | WH | 6798 | Camera video Signal | 4 | WH | 6798 | Camera video Signal
5 | YE | 6799 | Camera Shield | 5 | YE | 6799 | Camera Shield
6 | -- | -- | Not Used | 6 | -- | -- | Not Used