For 1990-2009 cars

Table 1: | Fluid Pump with Valve Trains Assemble
Table 2: | Torque Converter Fluid Seal and Fluid Filter Assembly Assemble

### Fluid Pump with Valve Trains Assemble

Callout | Component Name
--- | ---
1 | TCC Blow Off Ball Valve Train
2 | Pressure Regulator Valve Train
3 | Fluid Pump Blow Off Ball Valve Train
4 | TCC Control Valve Train
5 | Fluid Pump Drive Gear Tip The chamfer on the drive gear teeth face towards the pump body.
6 | Fluid Pump Driven Gear Tip The chamfer on the driven gear OD faces the pump body.
7 | Fluid Pump Cover
8 | Fluid Pump Cover Bolt M6 x 25 (Qty: 23) Caution: Refer to Fastener Caution in the Preface section. Tighten 12 N·m (106 lb in)

### Torque Converter Fluid Seal and Fluid Filter Assembly Assemble

Callout | Component Name
--- | ---
1 | Torque Converter Fluid Seal Assembly Tip The fluid seal assembly must be staked in place using DT-49131 tool to ensure proper seal retention.

#### Special Tools

• | DT-47792 Seal Installer

• | DT-49131 Seal Staking Tool

2 | Torque Converter Fluid Seal

#### Special Tools

DT-47791 Seal Installer

3 | Torque Converter Fluid Seal Retainer
4 | Fluid Filter Assembly Tip Rotate filter 90 degrees to engage locking tangs.