For 1990-2009 cars

## Door Window Guide Replacement Front

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the front door glass. Refer to Front Side Door Window Replacement.
3. Remove the power window regulator. Refer to Door Window Regulator Replacement.
4. Remove the bolts and the front window guide.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the front window guide with the bolts and tighten to 10 N·m (89 lb in).
2. Install the power window regulator. Refer to Door Window Regulator Replacement.
3. Install the front door glass. Refer to Front Side Door Window Replacement.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

## Door Window Guide Replacement Rear C100/Long Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the rear door glass. Refer to Rear Side Door Window Replacement.
3. Remove the power window regulator. Refer to Door Window Regulator Replacement.
4. Remove the rear door upper trim.
5. Remove the bolt and the nut, rear window guide.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear window guide with the bolt and the nut and tighten to 10 N·m (89 lb in).
2. Install the rear door upper trim.
3. Install the power window regulator. Refer to Door Window Regulator Replacement.
4. Install the rear door glass. Refer to Rear Side Door Window Replacement.
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

## Door Window Guide Replacement Rear C105/Short Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the rear door glass. Refer to Rear Side Door Window Replacement.
3. Remove the power window regulator. Refer to Door Window Regulator Replacement.
4. Remove the rear door upper trim.
5. Remove the bolt and the rear window guide.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear window guide with the bolt and tighten to 10 N·m (89 lb in).
2. Install the rear door upper trim.
3. Install the power window regulator. Refer to Door Window Regulator Replacement.
4. Install the rear door glass. Refer to Rear Side Door Window Replacement.
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.