For 1990-2009 cars

## Scan Tool Data List Except Holden

The electronic brake control module (EBCM) Scan Tool Data Lists contain all the antilock brake system related parameters that are available on the scan tool. The parameters in the list are arranged in alphabetical order. The column, "Data List," indicates the location of the parameter within the scan tool menu selections.

Use the EBCM Scan Tool Data Lists as directed by a diagnostic table or in order to supplement the diagnostic procedures. Begin all the diagnostic procedures with the antilock brake system (ABS) Diagnostic Starting Point. Use the EBCM Scan Tool Data Lists only after the following is determined:

• | There is no published DTC procedure nor published symptom procedure for the customer concern.

| OR

• | The DTC or symptom diagnostic procedure indicated by the diagnostic system check does not resolve the customer concern.

The Typical Data Values are obtained from a properly operating vehicle under the conditions specified in the first row of the Scan Tool Data List table. Comparison of the parameter values from the suspect vehicle with the Typical Data Values may reveal the source of the customer concern.

The ID Information menu is located on the EBCM main screen.

#### EBCM Scan Tool Data List

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition is ON, engine OFF, and vehicle is stationary
ABS Active | ABS | Yes/No | No
ABS Failed | ABS | On/Off | Off
ABS Warning Lamp | ABS | On/Off | Off
Battery Voltage Signal | ABS | Volts | B+
BPP Signal | ABS | Released/Applied | Released
Brake Fluid Level Status | ABS | OK/Low | OK
Brake Pressure Sensor Input | ABS | Volts | 0
Delivered Torque | ABS | % | 0-100%
DRP Active | ABS | Yes/No | No
DRP Disabled | ABS | Yes/No | No
Engine Drag Control Active | ABS | No/Yes | No
Engine Drag Control Failed | ABS | No/Yes | No
Lateral Accelerometer Signal | ABS | Volts | 2.5 Volts
LF Inlet Solenoid Command | ABS | Active/Inactive | Inactive
LF Outlet Solenoid Command | ABS | Active/Inactive | Inactive
LF Wheel Speed Sensor | ABS | km/h or mph | 0
Low Tire Pressure Lamp | ABS | On/Off | Off
LR Inlet Solenoid Command | ABS | Active/Inactive | Inactive
LR Outlet Solenoid Command | ABS | Active/Inactive | Inactive
LR Wheel Speed Sensor | ABS | km/h or mph | 0
Panic Brake Assist Failed | ABS | No/Yes | No
Pump Motor Command Voltage | ABS | B+/0 | B+
Requested Torque | ABS | % | 0-100%
RF Inlet Solenoid | ABS | Active/Inactive | Inactive
RF Outlet Solenoid | ABS | Active/Inactive | Inactive
RF Wheel Speed Sensor | ABS | km/h or mph | 0
RR Inlet Solenoid Command | ABS | Active/Inactive | Inactive
RR Outlet Solenoid Command | ABS | Active/Inactive | Inactive
RR Wheel Speed Sensor | ABS | km/h or mph | 0
Steering Wheel Position | ABS | Degrees | Varies 0-360
TCS Active | ABS | No/Yes | No
TCS Failed | ABS | No/Yes | No
TCS Warning Lamp | ABS | On/Off | Off
VSES Active | ABS | Yes/No | Yes
VSES Failed | ABS | Yes/No | No
Yaw Rate Sensor | ABS | Volts | 2.5 Volts

## Scan Tool Data List Holden

The electronic brake control module (EBCM) Scan Tool Data Lists contain all the antilock brake system related parameters that are available on the scan tool. The parameters in the list are arranged in alphabetical order.

Use the EBCM Scan Tool Data Lists as directed by a diagnostic table or in order to supplement the diagnostic procedures. Begin all the diagnostic procedures with the antilock brake system (ABS) Diagnostic Starting Point. Use the EBCM Scan Tool Data Lists only after the following is determined:

• | There is no published DTC procedure nor published symptom procedure for the customer concern.

| OR

• | The DTC or symptom diagnostic procedure indicated by the diagnostic system check does not resolve the customer concern.

The Typical Data Values are obtained from a properly operating vehicle under the conditions specified in the first row of the Scan Tool Data List table. Comparison of the parameter values from the suspect vehicle with the Typical Data Values may reveal the source of the customer concern.

Important: Do not use a scan tool that displays faulty data. The scan tool concern should be reported to the manufacturer. Use of a faulty scan tool may result in misdiagnosis and unnecessary parts replacement.

The ID Information menu is located on the EBCM main screen.

#### Scan Tool Data List

Scan Tool Parameter | System State | Expected Value | Description
--- | --- | --- | ---
Engine Idling / Operating Temperature / Closed Throttle / Park or Neutral / Closed Loop / Accessories Off
ABS Active | Yes No | - | The scan tool displays Yes/No. The scan tool displays No when not active.
ABS Failed (Anti-Lock Brake System) | Yes No | - | The scan tool will display Yes/No depending on the state of the ABS indicator.
ABS Telltale | On Off | - | This parameter displays On/Off. depending on the state of the ABS indicator.
Brake Fluid Level | OK Not OK | - | This parameter displays the status of the Brake Fluid Level.
Brake Light Switch | Active 12V Inactive 0V | - | This parameter displays the status of the Brake Light Switch.
Brake Pressure Sensor | - | bar | This parameter displays the Brake Pressure Sensor.
EBD Active (Electronic Brake Distribution) | Yes No | - | This parameter displays the status of the EBD Active and EBD Disabled.
EBD Disabled (Electronic Brake Distribution) | Yes No | -
ESP Active (Electronic Stability Program) | Yes No | - | This parameter displays the status of the ESP Active and ESP Failed.
ESP Failed (Electronic Stability Program) | Yes No | -
FL Hold Solenoid Commanded (Front Left) | Active | - | This parameter displays Active or Inactive. The scan tool displays the commanded state of the Hold Solenoids.
FR Hold Solenoid Commanded (Front Right)
RL Hold Solenoid Commanded (Rear Left) | Inactive
RR Hold Solenoid Commanded (Rear Right)
FL Release Solenoid Commanded (Front Left) | Active | - | This parameter displays Active or Inactive. The scan tool displays the commanded state of the Release Solenoids.
FR Release Solenoid Commanded (Front Right)
RL Release Solenoid Commanded (Rear Left) | Inactive
RR Release Solenoid Commanded (Rear Right)
FL Wheel Speed (Front Left) | - | km/h | This parameter displays each of the 4 wheel speed senors. The scan tool displays the actual speed of each wheel.
FR Wheel Speed (Front Right)
RL Wheel Speed (Rear Left)
RR Wheel Speed (Rear Right)
FL/RR TC/ESP Primary Solenoid Valve (Front Left/Rear Right) | Active Inactive | - | This parameter displays Active or Inactive. The scan tool displays the commanded state of the Primary solenoid valves.
FR/RL TC/ESP Primary Solenoid Valve (Front Right/Rear Left) | Active Inactive | -
FL/RR TC/ESP Switch Over Solenoid Valve (Front Left/Rear Right) | Active Inactive | - | This parameter displays Active or Inactive. The scan tool displays the commanded state of the Switch over solenoid valves.
FR/RL TC/ESP Switch Over Solenoid Valve (Front Right/Rear Left) | Active Inactive | -
Lateral Acceleration Sensor | - | m/s2 | This parameter displays the Lateral Acceleration Sensor.
Longitudinal Acceleration Sensor | - | m/s2 | This parameter displays the Longitudinal Acceleration Sensor.
Low Tire Pressure Lamp | On Off | - | This parameter displays the status of the Low Tire Pressure Lamp.
Panic Brake Assist Failed | Yes No | - | This parameter displays the status of the Panic Brake Assist Failed.
Pump Voltage | - | V | This parameter will display Voltage when the pump motor is active.
SAS Calibrated (Steering Angle Sensor) | Yes No | - | This parameter displays the status of the SAS Calibrated.
Steering Wheel Position | - | ° | This parameter displays the Steering Wheel Position.
System Voltage | - | V | This parameter displays Volts. The voltage measured between the module’s battery positive voltage circuit and ground circuit.
TC/ESP Telltale | On Off | - | This parameter displays On or Off. The scan tool displays On if the TC/ESP indicator is currently being commanded ON.
Traction Control Active | Yes No | - | This parameter displays the status of the Traction Control Active.
Traction Control Failed | Yes No | - | This parameter displays the status of the Traction Control Failed.
Yaw Rate Sensor | - | °/sec | This parameter displays the Yaw Rate Sensor.