For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the headlamp assembly. Refer to Headlamp Replacement.
3. Disconnect the electrical connector.
4. Remove the bolt and the horn.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the horn with the bolt and tighten to 20 N·m (15 lb ft).
2. Connect the electrical connector.
3. Install the headlamp assembly. Refer to Headlamp Replacement.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.