For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Steering Wheel and Column Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Steering Wheel and Column Description and Operation
2 | Verify that the steering column is loose. Is the steering column loose? | Go to Step 3 | System OK
3 | Inspect the steering column mounting brackets for looseness. Are the steering column mounting brackets loose? | Go to Step 6 | Go to Step 4
4 | Verify that the steering column bracket capsule is not sheared. Is the steering column bracket capsule sheared? | Go to Step 7 | Go to Step 5
5 | Inspect the intermediate shaft for worn joints or looseness. Is the intermediate joint worn or loose? | Go to Step 8 | Go to Step 9
6 | Caution: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten the mounting bolts to specifications. Refer to Fastener Tightening Specifications.

Did you complete the repair?

Go to Step 9

--

7 | Replace the steering column. Refer to Steering Column Replacement. Did you complete the replacement? | Go to Step 9 | --
8 | Tighten or replace the intermediate shaft as needed. Refer to Intermediate Steering Shaft Replacement. Did you complete the repair? | Go to Step 9 | --
9 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3