For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the front door lamp lens cover.
3. Remove the front door lamp.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the replacement front door lamp bulb.
3. Install the front door lamp lens cover.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.