For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

Important: Hold the link with a wrench during nut removal.

2. Remove the stabilizer link to stabilizer shaft nuts.
3. Remove the stabilizer shaft clamp bolts.
4. Remove the stabilizer shaft from the stabilizer link ball studs, while removing the stabilizer shaft from the vehicle.

### Installation Procedure

1. Position the stabilizer shaft in the vehicle, while installing the links on the stabilizer shaft.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the stabilizer shaft clamp bolts.

Tighten
Tighten the bolts to 70 N·m (52 lb ft).

Important: Hold the link with a wrench during nut installation.

3. Install the stabilizer link to stabilizer shaft nuts.

Tighten
Tighten the nuts to 57 N·m (42 lb ft).

4. Lower the vehicle.