For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Brake Pads

- New Lining Thickness

10.50 mm

0.413 in

- Minimum Lining Thickness

2.00 mm

0.079 in

Front Brake Rotors

- Diameter

296 mm

11.7 in

- New Thickness

29.00 mm

1.142 in

- Discard Thickness

27.40 mm

1.079 in

- Maximum Assembled Lateral Runout

0.04 mm

0.002 in

- Maximum Groove Depth

0.40 mm

0.016 in

- Maximum Thickness Variation

1.0 mm

0.04 in

Rear Brake Pads

- New Lining Thickness

9.00 mm

0.354 in

- Minimum Lining Thickness

2.00 mm

0.079 in

Rear Brake Rotors

- Diameter

303 mm

11.9 in

- New Thickness

20.00 mm

0.787 in

- Discard Thickness

18.40 mm

0.724 in

- Maximum Assembled Lateral Runout

0.04 mm

0.002 in

- Maximum Groove Depth

0.40 mm

0.016 in

- Maximum Thickness Variation

1.00 mm

0.04 in