For 1990-2009 cars

### Removal Procedure

1. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.
2. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
3. Rotate the accessory drive belt tensioner clockwise to reduce the belt tension.
4. While holding the tensioner in the reduced tension position, disconnect the belt.
5. Loosen the accessory drive belt idler pulley-to-generator through bolt.
6. Carefully support the generator and remove the generator upper mounting bolts to ease the removal of the through bolt.
7. Remove the accessory drive bolt idler pulley-to-generator through bolt.
8. Remove the accessory drive belt idler pulley.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Carefully support the generator and install the accessory drive belt idler pulley. Tighten the accessory drive belt idler pulley-to-generator through bolt to 50 N·m (37 lb ft).
2. Install the generator upper mounting bolts and tighten to 58 N·m (43 lb ft).
3. Rotate the accessory drive belt tensioner clockwise.
4. While holding the tensioner in the reduced tension position, install the belt.
5. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement
6. Install the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement