For 1990-2009 cars

### Removal Procedure

1. Remove the bolt (2) and the lower seat belt anchor (1).
2. Remove the lower center pillar trim panel. Refer to Center Pillar Lower Garnish Molding Replacement.
3. Remove the cap to reveal the upper seat belt anchor (2).
4. Remove the screws (3) and the seat belt guide (4).
5. Remove the bolt (1) and the upper seat belt anchor (2).
6. Remove the screw (1) from the seat belt retractor bracket.
7. Remove the bolt (3) and the seat belt retractor (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the seat belt retractor (2) with the bolt (3) and tighten to 38 N·m (28 lb ft).
2. Install the seat belt retractor bracket screw (1) and tighten to 10 N·m (7 lb ft).
3. Install the upper seat belt anchor (2) with the bolt (1) and tighten to 38 N·m (28 lb ft).
4. Install the seat belt guide (4) with the screws (3) and tighten to 3 N·m (27 lb in).
5. Install the seat belt guide anchor cap.
6. Install the lower center pillar trim panel. Refer to Center Pillar Lower Garnish Molding Replacement.
7. Install the lower seat belt anchor (1) with the bolt (2) and tighten to 38 N·m (28 lb ft).