For 1990-2009 cars

### Removal Procedure

1. Remove the center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement.
2. Remove the screws holding the shift indicator to the center console trim bezel and disconnect the electrical connector.
3. Remove the shift indicator from the center trim bezel.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Align the shift indicator with the center trim bezel and fasten with the screws and tighten to 2 N·m (18 lb in).
2. Connect the electrical connection to the center trim bezel.
3. Install the center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement.