For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.

Note: Hold the link with a wrench during nut removal.

3. Remove the stabilizer link to lower control arm nut.
4. Remove the trailing arm bracket to underbody bolts.

Warning: To prevent personal injury and/or component damage, use the proper tools to support the lower control arm when removing the coil spring. The coil spring is under extreme pressure and can become a projectile should the spring separate from the lower control arm before all of the tension is relieved.

5. Place a screw-type jack under the lower control arm.
6. Using the jack, compress the coil spring.
7. Remove the lower shock bolt.
8. Loosen the lower control arm to support frame bolt.
9. Remove the lower control arm to knuckle nut and bolt.
10. Lower the control arm in order to unload the coil spring.
11. Remove the coil spring and the insulators.

### Installation Procedure

1. Fully seat the top and bottom insulators to the coil spring.
2. Install the coil spring with the insulators to the lower control arm.
3. Using the screw type jack under the lower control arm, compress the coil spring.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the knuckle to the lower control arm and tighten.

• | The lower control arm to knuckle bolt to 160 N·m (118 lb ft).

• | The lower control arm to support nut and bolt.

• | The bolt to 110 N·m (81 lb ft).

5. Install the shock to the lower control arm and tighten to 110 N·m (81 lb ft).
6. Remove the jack.

Note: Hold the link with a wrench during nut installation.

7. Install the stabilizer link to the lower control arm and tighten to 15 N·m (11 lb ft).
8. Push the trailing arm upward in order to align the front bracket to body bolt.
9. Use a drift in order to aid in bracket alignment.
10. Install the bracket to body bolts and tighten to 110 N·m (81 lb ft).
11. Install the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
12. Lower the vehicle.
13. Measure the wheel alignment. Adjust the alignment if necessary. Refer to Wheel Alignment Measurement.