For 1990-2009 cars

1. Disassemble the engine block. Refer to Engine Block Disassemble.
2. Mark and confirm the connecting rod cap position to ensure they are installed in the same position for assembly.
3. Remove the connecting rod caps and bolts. Refer to Piston, Connecting Rod, and Bearing Removal.
4. Remove the lower crankcase. Refer to Lower Crankcase Replacement.

Important: Check and confirm the crankshaft bearing sequence to not confuse.

5. Remove the crankshaft and main bearings with the crankshaft oil seal.
6. Remove the oil nozzle tube.
7. Remove the CPS target wheel.