For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Fluid Reservoir Bolts | 9 N·m | 80 lb in
High-Pressure Hose Fitting | 28 N·m | 21 lb ft
Hydraulic Cylinder Line Fittings - Cylinder End | 19 N·m | 14 lb ft
Hydraulic Cylinder Line Fittings - Valve End | 19 N·m | 14 lb ft
Intermediate Shaft Pinch Bolts - Upper and Lower | 34 N·m | 25 lb ft
Outer Tie Rod Adjusting Nut | 60 N·m | 44 lb ft
Outer Tie Rod Nuts | 50 N·m | 37 lb ft
Power Steering Pump Bolts | 25 N·m | 18 lb ft
Power Steering Pump Bracket Bolts - Right Side | 25 N·m | 18 lb ft
Power Steering Pump Pressure Line Fitting | 28 N·m | 21 lb ft
Pressure Pipe Securing Bracket Bolts | 10 N·m | 88.5 lb in
SSPS Control Module Bracket Bolts | 10 N·m | 88.5 lb in
Steering Gear Inlet and Outlet Pipe Fittings | 28 N·m | 21 lb ft
Steering Gear Mounting Bolts | 110 N·m | 81 lb ft
Supply Pipe Securing Bracket Bolts | 10 N·m | 88.5 lb in