For 1990-2009 cars

### Removal Procedure

1. Remove the front wheel hub and bearing assembly. Refer to Front Wheel Bearing and Hub Replacement .
2. Remove the splash shield from the knuckle.

### Installation Procedure

1. Install the splash shield to the knuckle.
2. Secure the splash shield between the knuckle and the front wheel hub and bearing assembly. Refer to Front Wheel Bearing and Hub Replacement .