For 1990-2009 cars

### Removal Procedure

Caution: Ensure that the vehicle is properly supported and squarely positioned. To help avoid personal injury when a vehicle is on a hoist, provide additional support for the vehicle on the opposite end from which the components are being removed.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the engine protection shield. Refer to Engine Shield Replacement .
3. support the powertrain with a suitable jack stand.
4. Remove the front transmission mount to frame bolt (1).
5. Remove the front transmission mount to transmission bolts (1).
6. Remove the front transmission mount (2).

### Installation Procedure

1. Install the front transmission mount (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the front transmission mount to transmission bolts (1) and tighten to 50 N·m (37 lb ft) .
3. Install the front transmission mount to frame bolt (1) and tighten to 90 N·m (66 lb ft) .
4. Remove the jack stand supporting the powertrain.
5. Install the engine protection shield. Refer to Engine Shield Replacement .
6. Lower the vehicle .