For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the steering column cover. Refer to Steering Column Trim Covers Replacement .
3. Disconnect the electrical connector.
4. Remove the key hole lamp retaining screw.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the key hole lamp retaining screw.

Tighten
Tighten the key hole lamp retaining screw to 2.5 N·m (22 lb in).

2. Connect the electrical connector.
3. Install the steering column cover. Refer to Steering Column Trim Covers Replacement .
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .