For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Perform an initial inspection of the power steering system. Is the system operational? | -- | Go to Step 2 | Go to Diagnostic Starting Point - Power Steering System
2 |

1. Install a scan tool.
2. Turn ON the ignition.
3. Check the DTC code by using scan tool.

Does the scan tool display any DTCs?

--

Go to Diagnostic Trouble Code (DTC) List - Vehicle

Go to Step 3

3 | Check for a poor connection at the ABS control module. Did you find and correct the condition? | -- | System OK | Go to Step 4
4 |

1. Turn OFF the ignition.
2. Disconnect the connector of control module wiring.
3. Disconnect the connector of ABS control module.
4. Check the resistance between the terminal 6 of SSPS wiring connector and the terminal 3 of ABS wiring connector.

Is the resistance equal to the specified value?

0 ohms

Go to Step 5

Go to Step 6

5 | Replace of repair the damaged wiring. Is the repair complete? | -- | System OK | --
6 | Replace the SSPS control module. Is the replacement complete? | -- | System OK | --