For 1990-2009 cars

Checks | Actions
--- | ---
Check for a contaminated or warped flywheel. | Repair or replace the flywheel.
Check for a weak diaphragm spring. | Replace the necessary clutch components. Refer to Clutch Assembly Replacement .
Check for a oily contamination of the clutch disc. | Replace the necessary clutch components. Refer to Clutch Assembly Replacement .
Check for worn splines on the input shaft. | Replace the splines on the input shaft.