For 1990-2009 cars

### Removal Procedure

1. Remove the bolt and the upper front seat belt anchor.
2. Reposition the upper portion of the center pillar lower garnish molding.
3. Remove the screw and pry off the center pillar upper garnish molding.

### Installation Procedure

1. Install the center pillar upper garnish molding.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the upper portion of the center pillar lower garnish molding and tighten the screw to 22 N·m (16 lb ft).
3. Install the upper front seat belt anchor with the bolt and tighten to 38 N·m (28 lb ft).