For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the liftgate upper applique. Refer to Liftgate Upper Applique Replacement.
3. Disconnect the electrical connector.
4. Remove the CHMSL bulb.

### Installation Procedure

1. Install the replacement CHMSL bulb.
2. Connect the electrical connector.
3. Install the liftgate upper applique. Refer to Liftgate Upper Applique Replacement.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.