For 1990-2009 cars

### Removal Procedure

1. Remove the liftgate lower trim. Refer to Liftgate Trim Panel Replacement .
2. Remove the bolts and the liftgate window latch.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the liftgate window latch with the bolts.
3. Install the liftgate lower trim. Refer to Liftgate Trim Panel Replacement .