For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the intermediate drive shaft. Refer to Front Wheel Drive Shaft Replacement .

1 | Right Front Wheel Drive Shaft Oil Seal Tip

• | For seal removal use J-6125-B hammer with J-23129 remover .

• | For seal installation use J-8092 handle with DT-47790 installer .

#### Special Tools

• | DT-47790 Seal Installer

• | J-6125-B Slide Hammer

• | J-8092 Driver Handle

• | J-23129 Universal Seal Remover