For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the toe link to knuckle nut and bolt.
3. Remove the toe link to support nut and bolt.
4. Remove the toe link from the vehicle.

### Installation Procedure

1. Install the toe link to the support assembly.

Important:

• | Install the bolt with the head towards the front of the vehicle.

• | Position the cam nut in same position as in the upper control arm.

2. Install the toe link to support nut and bolt.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the toe link to the knuckle.

Tighten
Tighten the bolt to 160 N·m (118 lb ft).

4. Tighten the toe link to support bolt.

Tighten
Tighten the bolt to 160 N·m (118 lb ft).

5. Lower the vehicle.
6. Check the rear alignment. Refer to Wheel Alignment Measurement .