For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Torque Converter and Differential Housing Seal
2 | Fluid Pump Assembly
3 | Fluid Pump Bolt M8 x 33 (Qty: 8) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in) then rotate the bolt an additional 45 degrees.

#### Special Tools

J-45059 Angle Meter or equivalent

4 | Front Differential Ring Gear
5 | Front Differential Ring Gear Retainer Tip Install the retainer with the taper facing away from the ring gear.
6 | Front Differential Carrier Baffle
7 | Front Differential Carrier Baffle Bolt M6 x 25 (Qty: 2) Tighten 12 N·m (106.21 lb in)