For 1990-2009 cars

## Outer Belt Sealing Strip Replacement C 100/Long Body

### Removal Procedure

1. Lower the window completely.
2. Remove the window outer sealing strip screw.
3. Remove the outside rearview mirror. Refer to Outside Rearview Mirror Replacement .
4. Lift the window outer sealing strip off the door.

### Installation Procedure

1. Press the outside channel molding onto the door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the window outer sealing strip screw.

Tighten
Tighten the window outer sealing strip screw to 1.3 N·m (12 lb in).

3. Install the outside rearview mirror. Refer to Outside Rearview Mirror Replacement .
4. Raise the window.

## Outer Belt Sealing Strip Replacement C 105/Short Body

### Removal Procedure

1. Lower the window completely.
2. Remove the window outer sealing strip screws.
3. Remove the outside rearview mirror. Refer to Outside Rearview Mirror Replacement .
4. Lift the window outer sealing strip off the door.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Press the outside channel molding onto the door.
2. Install the window outer sealing strip screws.

Tighten
Tighten the window outer sealing strip screws to 1.3 N·m (12 lb in).

3. Install the outside rearview mirror. Refer to Outside Rearview Mirror Replacement .
4. Raise the window.