For 1990-2009 cars

### Removal Procedure

1. Discharge the A/C (Air Conditioning) system, if equipped.
2. Remove the radiator grille guide and grille. Refer to Grille Replacement .
3. Remove the engine under cover. Refer to Engine Shield Replacement .
4. Remove the hood primary latch support. Refer to Hood Primary Latch Replacement .
5. Remove the charge air cooler inlet/outlet hoses. Refer to Charge Air Cooler Inlet Pipe and Outlet Pipe Replacement .
6. Remove the A/C condenser from the radiator. Refer to Condenser Replacement .
7. Remove the radiator upper bracket.
8. Remove the charge air cooler bolts.
9. Remove the charge air cooler.

### Installation Procedure

1. Install the charge air cooler to the radiator.
2. Install the charge air cooler bolts.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the radiator upper bracket.

Tighten

• | Tighten the charge air cooler bolts to 8.5 N·m (75.2 lb in).

• | Tighten the radiator upper bracket bolts to 20 N·m (14.8 lb ft).