For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the map lamp assembly. Refer to Reading Lamp Replacement .
3. Disconnect the electrical connector from the intrusion sensor.
4. Remove the screws and the intrusion sensor bracket.
5. Remove the intrusion sensor.

### Installation Procedure

1. Install the intrusion sensor.
2. Install the intrusion sensor bracket and screws.
3. Connect the electrical connector to the intrusion sensor.
4. Install the map lamp assembly. Refer to Reading Lamp Replacement .
5. Connect the negative battery cable.