For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Roof Console Assembly

#### Procedure

1. Use a flat-bladed tool on the bezel to release the tabs and gently pull down to remove the roof console.
2. Disconnect the electrical connectors.
3. If replacing the roof console assembly, transfer all necessary components.
4. Uplevel console shown, all others similar and are removed in the same manner.

2 | Roof Console Retainer (Qty: 4)