For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front side door window frame rear applique. Refer to Front Door Frame Applique Replacement .
3. Remove the screws that secure the glass to the window regulator.
4. Remove the glass from the door.

### Installation Procedure

1. Install the glass in the door and position the glass within the window regulator.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the glass to the window regulator with the screws.

Tighten
Tighten the glass screws to 3 N·m (27 lb in).

3. Install the front side door window frame rear applique. Refer to Front Door Frame Applique Replacement .
4. Install the front door trim. Refer to Front Side Door Trim Panel Replacement .