For 1990-2009 cars

For step by step programming instructions, please refer to the techline information system (TIS) terminal.

Review the information below to ensure proper programming protocol.

Important:

• | DO NOT program a control module unless you are directed by a service procedure or you are directed by a General Motors Corporation service bulletin. Programming a control module at any other time will not permanently correct a customer's concern.

• | It is essential that the Tech 2 and the TIS terminal are both equipped with the latest software before performing service programming system (SPS).

• | Some modules will require additional programming/setup events performed before or after programming.

• | Some vehicles may require the use of a CANDi module for programming.

• | Review the appropriate service information for these procedures.

• | DTCs may set during programming. Clear DTCs after programming is complete.

• | Clearing powertrain DTCs will set the Inspection/Maintenance (I/M) system status indicators to NO.

Ensure the following conditions are met before programming a control module:

• | Vehicle system voltage

- | There is not a charging system concern. All charging system concerns must be repaired before programming a control module.

- | Battery voltage is greater than 12 volts but less than 16 volts. The battery must be charged before programming the control module if the battery voltage is low.

- | A battery charger is NOT connected to the vehicle's battery. Incorrect system voltage or voltage fluctuations from a battery charger, may cause programming failure or control module damage.

- | Turn OFF or disable any system that may put a load on the vehicle's battery, such as the following components:

• | Twilight sentinel

• | Interior lights

• | Daytime running lights (DRL)--Applying the parking brake, on most vehicles, disables the DRL system. Refer to the Owner's manual.

• | Heating, ventilation, and air conditioning (HVAC) systems

• | Engine cooling fans, radio, etc.

• | The ignition switch must be in the proper position. The Tech 2 prompts you to turn ON the ignition, with the engine OFF. DO NOT change the position of the ignition switch during the programming procedure, unless instructed to do so.

• | Make certain all tool connections are secure, including the following components and circuits:

- | The RS-232 communication cable port

- | The connection at the data link connector (DLC)

- | The voltage supply circuits

• | DO NOT disturb the tool harnesses while programming. If an interruption occurs during the programming procedure, programming failure or control module damage may occur.

• | DO NOT turn OFF the ignition if the programming procedure is interrupted or unsuccessful. Ensure that all control module and DLC connections are secure and the TIS terminal operating software is up to date. Attempt to reprogram the control module. If the control module cannot be programmed, replace the control module.