For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Steering Wheel and Column Description and perform the necessary inspections? | Go to Step 2 | Go to Steering Wheel and Column Description and Operation
2 | Verify that noise is present in the steering column during operation. Is noise present in the steering column during operation? | Go to Step 3 | System OK
3 | Inspect the steering column components for looseness. Are the steering column components loose? | Go to Step 6 | Go to Step 4
4 | Inspect the SIR coil for noise. Is the SIR coil noisy? | Go to Step 7 | Go to Step 5
5 | Inspect the upper steering column shaft bearing for the following conditions:

• | Damage

• | Lubrication

• | Wear

• | Proper seating

Are the bearings in need of repair or replacement?

Go to Step 8

Go to Step 9

6 | Tighten the steering column components to specifications. Refer to Fastener Tightening Specifications . Did you complete the repair? | Go to Step 9 | --
7 | Replace the SIR coil. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement . Did you complete the repair? | Go to Step 9 | --
8 | Replace the steering column. Refer to Steering Column Replacement . Did you complete the repair? | Go to Step 9 | --
9 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3