For 1990-2009 cars

#### Tools Required

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

1. Remove the battery and battery tray. Refer to Battery Tray Replacement .

Important: Only lift the engine far enough to take the weight off the transaxle mount assembly.

2. Support the engine assembly using the DW-110-060 .
3. Remove the transaxle mount bracket retaining bolts from the transaxle.
4. Remove the transaxle mount assembly retaining bolts from the left front longitudinal.
5. Remove the transaxle mount assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the transaxle mount assembly.

Tighten

• | Tighten the transaxle mount assembly retaining bolts (2) to 37 N·m (27 lb ft).

• | Tighten the transaxle mount bracket retaining bolts (1) to 50 N·m (37 lb ft).

2. Remove the DW-110-060 .
3. Install the battery and battery tray. Refer to Battery Tray Replacement .