For 1990-2009 cars

## Headlamp Leveling Switch Replacement C 100/Long Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the instrument cluster steering column opening pillar.
3. Remove the screw and the headlamp leveling switch.
4. Disconnect the electrical connectors.

### Installation Procedure

1. Replace the appropriate switch.
2. Connect the electrical connectors.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the headlamp leveling switch with the screw.

Tighten
Tighten the headlamp leveling switch screws to 2 N·m (18 lb in).

4. Install the instrument cluster steering column opening pillar.
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .

## Headlamp Leveling Switch Replacement C 105/Short Body

### Removal Procedure

Important: Left - Hand Drive Shown, Right - Hand Drive Similar.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the instrument cluster steering column opening pillar.
3. Remove the screw and the headlamp leveling switch.
4. Disconnect the electrical connectors.

### Installation Procedure

1. Replace the appropriate switch.
2. Connect the electrical connectors.
3. Install the headlamp leveling switch with the screw.

Tighten
Tighten the headlamp leveling switch screws to 2 N·m (18 lb in).

4. Install the instrument cluster steering column opening pillar.
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .