For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable.
2. Remove the instrument panel (I/P) center trim panel.
3. Remove the screws and the audio system.
4. Disconnect the audio system electrical connectors.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Connect the audio system electrical connectors.
2. Install the audio system with the screws and tighten to 4 N·m (35 lb in).
3. Install the I/P center trim panel.
4. Connect the negative battery cable.