For 1990-2009 cars

### Removal Procedure

Note: The left-hand drive is shown. The right-hand drive is similar.

1. Open the hood.
2. Remove the nuts to access wiper arm nut from the wiper arm.
3. Lift wiper arm assembly away from windshield and remove wiper arm from pivot shaft.

### Installation Procedure

1. Install the wiper arm.

Caution: Refer to Fastener Caution in the Preface section.

2. Secure the wiper arm with the nut and tighten to 22 N·m (16 lb ft).
3. Operate the windshield wipers and inspect for proper operation.
4. Close the hood.