For 1990-2009 cars

1. Raise and support the vehicle.
2. Remove the transaxle drain plug and allow the transaxle to drain completely.
3. Remove the fluid level check plug.

Caution: Refer to Fastener Caution in the Preface section.

4. Clean and install the transaxle drain plug and tighten to 6 N·m (53 lb in) plus an additional 45-180 degrees.
5. Add SAE75W90 transaxle fluid until it seeps out of the fluid level check plug.
6. Clean and install the fluid level check plug and tighten to 6 N·m (53 lb in) plus an additional 45-180 degrees.
7. Lower the vehicle and verify proper operation.

Fluid Specification | SAE75W90
--- | ---
Fluid Capacity | FWD | 2.1L (2.22 qt)