For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement .
2. Remove the screws and the driver information bezel.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the driver information bezel with the screws.

Tighten
Tighten the driver information bezel screws to 2 N·m (18 lb in).

2. Install the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement .