For 1990-2009 cars

### Removal Procedure

1. Remove the bolt and the upper front seat belt anchor.
2. Reposition the upper portion of the center pillar lower garnish molding.
3. Remove the screw and pry off the center pillar upper garnish molding.

### Installation Procedure

1. Install the center pillar upper garnish molding.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the upper portion of the center pillar lower garnish molding.

Tighten
Tighten the center pillar lower garnish molding screw to 22 N·m (16 lb ft).

3. Install the upper front seat belt anchor with the bolt.

Tighten
Tighten the seat belt anchor bolt to 38 N·m (28 lb ft).